----------------------------------------------------------------------
1. INTRODUCTION

Modern filesystems feature checksumming of data and metadata to
protect against data corruption.  However, the detection of the
corruption is done at read time which could potentially be months
after the data was written.  At that point the original data that the
application tried to write is most likely lost.

The solution is to ensure that the disk is actually storing what the
application meant it to.  Recent additions to both the SCSI family
protocols (SBC Data Integrity Field, SCC protection proposal) as well
as SATA/T13 (External Path Protection) try to remedy this by adding
support for appending integrity metadata to an I/O.  The integrity
metadata (or protection information in SCSI terminology) includes a
checksum for each sector as well as an incrementing counter that
ensures the individual sectors are written in the right order.  And
for some protection schemes also that the I/O is written to the right
place on disk.

Current storage controllers and devices implement various protective
measures, for instance checksumming and scrubbing.  But these
technologies are working in their own isolated domains or at best
between adjacent nodes in the I/O path.  The interesting thing about
DIF and the other integrity extensions is that the protection format
is well defined and every node in the I/O path can verify the
integrity of the I/O and reject it if corruption is detected.  This
allows not only corruption prevention but also isolation of the point
of failure.

----------------------------------------------------------------------
2. THE DATA INTEGRITY EXTENSIONS

As written, the protocol extensions only protect the path between
controller and storage device.  However, many controllers actually
allow the operating system to interact with the integrity metadata
(IMD).  We have been working with several FC/SAS HBA vendors to enable
the protection information to be transferred to and from their
controllers.

The SCSI Data Integrity Field works by appending 8 bytes of protection
information to each sector.  The data + integrity metadata is stored
in 520 byte sectors on disk.  Data + IMD are interleaved when
transferred between the controller and target.  The T13 proposal is
similar.

Because it is highly inconvenient for operating systems to deal with
520 (and 4104) byte sectors, we approached several HBA vendors and
encouraged them to allow separation of the data and integrity metadata
scatter-gather lists.

The controller will interleave the buffers on write and split them on
read.  This means that the Linux can DMA the data buffers to and from
host memory without changes to the page cache.

Also, the 16-bit CRC checksum mandated by both the SCSI and SATA specs
is somewhat heavy to compute in software.  Benchmarks found that
calculating this checksum had a significant impact on system
performance for a number of workloads.  Some controllers allow a
lighter-weight checksum to be used when interfacing with the operating
system.  Emulex, for instance, supports the TCP/IP checksum instead.
The IP checksum received from the OS is converted to the 16-bit CRC
when writing and vice versa.  This allows the integrity metadata to be
generated by Linux or the application at very low cost (comparable to
software RAID5).

The IP checksum is weaker than the CRC in terms of detecting bit
errors.  However, the strength is really in the separation of the data
buffers and the integrity metadata.  These two distinct buffers much
match up for an I/O to complete.

The separation of the data and integrity metadata buffers as well as
the choice in checksums is referred to as the Data Integrity
Extensions.  As these extensions are outside the scope of the protocol
bodies (T10, T13), Oracle and its partners are trying to standardize
them within the Storage Networking Industry Association.

----------------------------------------------------------------------
3. KERNEL CHANGES

The data integrity framework in Linux enables protection information
to be pinned to I/Os and sent to/received from controllers that
support it.

The advantage to the integrity extensions in SCSI and SATA is that
they enable us to protect the entire path from application to storage
device.  However, at the same time this is also the biggest
disadvantage. It means that the protection information must be in a
format that can be understood by the disk.

Generally Linux/POSIX applications are agnostic to the intricacies of
the storage devices they are accessing.  The virtual filesystem switch
and the block layer make things like hardware sector size and
transport protocols completely transparent to the application.

However, this level of detail is required when preparing the
protection information to send to a disk.  Consequently, the very
concept of an end-to-end protection scheme is a layering violation.
It is completely unreasonable for an application to be aware whether
it is accessing a SCSI or SATA disk.

The data integrity support implemented in Linux attempts to hide this
from the application.  As far as the application (and to some extent
the kernel) is concerned, the integrity metadata is opaque information
that's attached to the I/O.

The current implementation allows the block layer to automatically
generate the protection information for any I/O.  Eventually the
intent is to move the integrity metadata calculation to userspace for
user data.  Metadata and other I/O that originates within the kernel
will still use the automatic generation interface.

Some storage devices allow each hardware sector to be tagged with a
16-bit value.  The owner of this tag space is the owner of the block
device.  I.e. the filesystem in most cases.  The filesystem can use
this extra space to tag sectors as they see fit.  Because the tag
space is limited, the block interface allows tagging bigger chunks by
way of interleaving.  This way, 8*16 bits of information can be
attached to a typical 4KB filesystem block.

This also means that applications such as fsck and mkfs will need
access to manipulate the tags from user space.  A passthrough
interface for this is being worked on.


----------------------------------------------------------------------
4. BLOCK LAYER IMPLEMENTATION DETAILS

4.1 BIO

The data integrity patches add a new field to struct bio when
CONFIG_BLK_DEV_INTEGRITY is enabled.  bio->bi_integrity is a pointer
to a struct bip which contains the bio integrity payload.  Essentially
a bip is a trimmed down struct bio which holds a bio_vec containing
the integrity metadata and the required housekeeping information (bvec
pool, vector count, etc.)

A kernel subsystem can enable data integrity protection on a bio by
calling bio_integrity_alloc(bio).  This will allocate and attach the
bip to the bio.

Individual pages containing integrity metadata can subsequently be
attached using bio_integrity_add_page().

bio_free() will automatically free the bip.


4.2 BLOCK DEVICE

Because the format of the protection data is tied to the physical
disk, each block device has been extended with a block integrity
profile (struct blk_integrity).  This optional profile is registered
with the block layer using blk_integrity_register().

The profile contains callback functions for generating and verifying
the protection data, as well as getting and setting application tags.
The profile also contains a few constants to aid in completing,
merging and splitting the integrity metadata.

Layered block devices will need to pick a profile that's appropriate
for all subdevices.  blk_integrity_compare() can help with that.  DM
and MD linear, RAID0 and RAID1 are currently supported.  RAID4/5/6
will require extra work due to the application tag.


----------------------------------------------------------------------
5.0 BLOCK LAYER INTEGRITY API

5.1 NORMAL FILESYSTEM

    The normal filesystem is unaware that the underlying block device
    is capable of sending/receiving integrity metadata.  The IMD will
    be automatically generated by the block layer at submit_bio() time
    in case of a WRITE.  A READ request will cause the I/O integrity
    to be verified upon completion.

    IMD generation and verification can be toggled using the

      /sys/block/<bdev>/integrity/write_generate

    and

      /sys/block/<bdev>/integrity/read_verify

    flags.


5.2 INTEGRITY-AWARE FILESYSTEM

    A filesystem that is integrity-aware can prepare I/Os with IMD
    attached.  It can also use the application tag space if this is
    supported by the block device.


    int bdev_integrity_enabled(block_device, int rw);

      bdev_integrity_enabled() will return 1 if the block device
      supports integrity metadata transfer for the data direction
      specified in 'rw'.

      bdev_integrity_enabled() honors the write_generate and
      read_verify flags in sysfs and will respond accordingly.


    int bio_integrity_prep(bio);

      To generate IMD for WRITE and to set up buffers for READ, the
      filesystem must call bio_integrity_prep(bio).

      Prior to calling this function, the bio data direction and start
      sector must be set, and the bio should have all data pages
      added.  It is up to the caller to ensure that the bio does not
      change while I/O is in progress.

      bio_integrity_prep() should only be called if
      bio_integrity_enabled() returned 1.


    int bio_integrity_tag_size(bio);

      If the filesystem wants to use the application tag space it will
      first have to find out how much storage space is available.
      Because tag space is generally limited (usually 2 bytes per
      sector regardless of sector size), the integrity framework
      supports interleaving the information between the sectors in an
      I/O.

      Filesystems can call bio_integrity_tag_size(bio) to find out how
      many bytes of storage are available for that particular bio.

      Another option is bdev_get_tag_size(block_device) which will
      return the number of available bytes per hardware sector.


    int bio_integrity_set_tag(bio, void *tag_buf, len);

      After a successful return from bio_integrity_prep(),
      bio_integrity_set_tag() can be used to attach an opaque tag
      buffer to a bio.  Obviously this only makes sense if the I/O is
      a WRITE.


    int bio_integrity_get_tag(bio, void *tag_buf, len);

      Similarly, at READ I/O completion time the filesystem can
      retrieve the tag buffer using bio_integrity_get_tag().


6.3 PASSING EXISTING INTEGRITY METADATA

    Filesystems that either generate their own integrity metadata or
    are capable of transferring IMD from user space can use the
    following calls:


    struct bip * bio_integrity_alloc(bio, gfp_mask, nr_pages);

      Allocates the bio integrity payload and hangs it off of the bio.
      nr_pages indicate how many pages of protection data need to be
      stored in the integrity bio_vec list (similar to bio_alloc()).

      The integrity payload will be freed at bio_free() time.


    int bio_integrity_add_page(bio, page, len, offset);

      Attaches a page containing integrity metadata to an existing
      bio.  The bio must have an existing bip,
      i.e. bio_integrity_alloc() must have been called.  For a WRITE,
      the integrity metadata in the pages must be in a format
      understood by the target device with the notable exception that
      the sector numbers will be remapped as the request traverses the
      I/O stack.  This implies that the pages added using this call
      will be modified during I/O!  The first reference tag in the
      integrity metadata must have a value of bip->bip_sector.

      Pages can be added using bio_integrity_add_page() as long as
      there is room in the bip bio_vec array (nr_pages).

      Upon completion of a READ operation, the attached pages will
      contain the integrity metadata received from the storage device.
      It is up to the receiver to process them and verify data
      integrity upon completion.


6.4 REGISTERING A BLOCK DEVICE AS CAPABLE OF EXCHANGING INTEGRITY
    METADATA

    To enable integrity exchange on a block device the gendisk must be
    registered as capable:

    int blk_integrity_register(gendisk, blk_integrity);

      The blk_integrity struct is a template and should contain the
      following:

        static struct blk_integrity my_profile = {
            .name                   = "STANDARDSBODY-TYPE-VARIANT-CSUM",
            .generate_fn            = my_generate_fn,
       	    .verify_fn              = my_verify_fn,
       	    .get_tag_fn             = my_get_tag_fn,
       	    .set_tag_fn             = my_set_tag_fn,
	    .tuple_size             = sizeof(struct my_tuple_size),
	    .tag_size               = <tag bytes per hw sector>,
        };

      'name' is a text string which will be visible in sysfs.  This is
      part of the userland API so chose it carefully and never change
      it.  The format is standards body-type-variant.
      E.g. T10-DIF-TYPE1-IP or T13-EPP-0-CRC.

      'generate_fn' generates appropriate integrity metadata (for WRITE).

      'verify_fn' verifies that the data buffer matches the integrity
      metadata.

      'tuple_size' must be set to match the size of the integrity
      metadata per sector.  I.e. 8 for DIF and EPP.

      'tag_size' must be set to identify how many bytes of tag space
      are available per hardware sector.  For DIF this is either 2 or
      0 depending on the value of the Control Mode Page ATO bit.

      See 6.2 for a description of get_tag_fn and set_tag_fn.

----------------------------------------------------------------------
2007-12-24 Martin K. Petersen <martin.petersen@oracle.com>
