Regulator Consumer Driver Interface
===================================

This text describes the regulator interface for consumer device drivers.
Please see overview.txt for a description of the terms used in this text.


1. Consumer Regulator Access (static & dynamic drivers)
=======================================================

A consumer driver can get access to it's supply regulator by calling :-

regulator = regulator_get(dev, "Vcc");

The consumer passes in it's struct device pointer and power supply ID. The core
then finds the correct regulator by consulting a machine specific lookup table.
If the lookup is successful then this call will return a pointer to the struct
regulator that supplies this consumer.

To release the regulator the consumer driver should call :-

regulator_put(regulator);

Consumers can be supplied by more than one regulator e.g. codec consumer with
analog and digital supplies :-

digital = regulator_get(dev, "Vcc");  /* digital core */
analog = regulator_get(dev, "Avdd");  /* analog */

The regulator access functions regulator_get() and regulator_put() will
usually be called in your device drivers probe() and remove() respectively.


2. Regulator Output Enable & Disable (static & dynamic drivers)
====================================================================

A consumer can enable it's power supply by calling:-

int regulator_enable(regulator);

NOTE: The supply may already be enabled before regulator_enabled() is called.
This may happen if the consumer shares the regulator or the regulator has been
previously enabled by bootloader or kernel board initialization code.

A consumer can determine if a regulator is enabled by calling :-

int regulator_is_enabled(regulator);

This will return > zero when the regulator is enabled.


A consumer can disable it's supply when no longer needed by calling :-

int regulator_disable(regulator);

NOTE: This may not disable the supply if it's shared with other consumers. The
regulator will only be disabled when the enabled reference count is zero.

Finally, a regulator can be forcefully disabled in the case of an emergency :-

int regulator_force_disable(regulator);

NOTE: this will immediately and forcefully shutdown the regulator output. All
consumers will be powered off.


3. Regulator Voltage Control & Status (dynamic drivers)
======================================================

Some consumer drivers need to be able to dynamically change their supply
voltage to match system operating points. e.g. CPUfreq drivers can scale
voltage along with frequency to save power, SD drivers may need to select the
correct card voltage, etc.

Consumers can control their supply voltage by calling :-

int regulator_set_voltage(regulator, min_uV, max_uV);

Where min_uV and max_uV are the minimum and maximum acceptable voltages in
microvolts.

NOTE: this can be called when the regulator is enabled or disabled. If called
when enabled, then the voltage changes instantly, otherwise the voltage
configuration changes and the voltage is physically set when the regulator is
next enabled.

The regulators configured voltage output can be found by calling :-

int regulator_get_voltage(regulator);

NOTE: get_voltage() will return the configured output voltage whether the
regulator is enabled or disabled and should NOT be used to determine regulator
output state. However this can be used in conjunction with is_enabled() to
determine the regulator physical output voltage.


4. Regulator Current Limit Control & Status (dynamic drivers)
===========================================================

Some consumer drivers need to be able to dynamically change their supply
current limit to match system operating points. e.g. LCD backlight driver can
change the current limit to vary the backlight brightness, USB drivers may want
to set the limit to 500mA when supplying power.

Consumers can control their supply current limit by calling :-

int regulator_set_current_limit(regulator, min_uA, max_uA);

Where min_uA and max_uA are the minimum and maximum acceptable current limit in
microamps.

NOTE: this can be called when the regulator is enabled or disabled. If called
when enabled, then the current limit changes instantly, otherwise the current
limit configuration changes and the current limit is physically set when the
regulator is next enabled.

A regulators current limit can be found by calling :-

int regulator_get_current_limit(regulator);

NOTE: get_current_limit() will return the current limit whether the regulator
is enabled or disabled and should not be used to determine regulator current
load.


5. Regulator Operating Mode Control & Status (dynamic drivers)
=============================================================

Some consumers can further save system power by changing the operating mode of
their supply regulator to be more efficient when the consumers operating state
changes. e.g. consumer driver is idle and subsequently draws less current

Regulator operating mode can be changed indirectly or directly.

Indirect operating mode control.
--------------------------------
Consumer drivers can request a change in their supply regulator operating mode
by calling :-

int regulator_set_optimum_mode(struct regulator *regulator, int load_uA);

This will cause the core to recalculate the total load on the regulator (based
on all it's consumers) and change operating mode (if necessary and permitted)
to best match the current operating load.

The load_uA value can be determined from the consumers datasheet. e.g.most
datasheets have tables showing the max current consumed in certain situations.

Most consumers will use indirect operating mode control since they have no
knowledge of the regulator or whether the regulator is shared with other
consumers.

Direct operating mode control.
------------------------------
Bespoke or tightly coupled drivers may want to directly control regulator
operating mode depending on their operating point. This can be achieved by
calling :-

int regulator_set_mode(struct regulator *regulator, unsigned int mode);
unsigned int regulator_get_mode(struct regulator *regulator);

Direct mode will only be used by consumers that *know* about the regulator and
are not sharing the regulator with other consumers.


6. Regulator Events
===================
Regulators can notify consumers of external events. Events could be received by
consumers under regulator stress or failure conditions.

Consumers can register interest in regulator events by calling :-

int regulator_register_notifier(struct regulator *regulator,
			      struct notifier_block *nb);

Consumers can uregister interest by calling :-

int regulator_unregister_notifier(struct regulator *regulator,
				struct notifier_block *nb);

Regulators use the kernel notifier framework to send event to their interested
consumers.
