The additional fields in struct boot_params as a part of 32-bit boot
protocol of kernel. These should be filled by bootloader or 16-bit
real-mode setup code of the kernel. References/settings to it mainly
are in:

  arch/x86/include/asm/bootparam.h


Offset	Proto	Name		Meaning
/Size

000/040	ALL	screen_info	Text mode or frame buffer information
				(struct screen_info)
040/014	ALL	apm_bios_info	APM BIOS information (struct apm_bios_info)
060/010	ALL	ist_info	Intel SpeedStep (IST) BIOS support information
				(struct ist_info)
080/010	ALL	hd0_info	hd0 disk parameter, OBSOLETE!!
090/010	ALL	hd1_info	hd1 disk parameter, OBSOLETE!!
0A0/010	ALL	sys_desc_table	System description table (struct sys_desc_table)
140/080	ALL	edid_info	Video mode setup (struct edid_info)
1C0/020	ALL	efi_info	EFI 32 information (struct efi_info)
1E0/004	ALL	alk_mem_k	Alternative mem check, in KB
1E4/004	ALL	scratch		Scratch field for the kernel setup code
1E8/001	ALL	e820_entries	Number of entries in e820_map (below)
1E9/001	ALL	eddbuf_entries	Number of entries in eddbuf (below)
1EA/001	ALL	edd_mbr_sig_buf_entries	Number of entries in edd_mbr_sig_buffer
				(below)
290/040	ALL	edd_mbr_sig_buffer EDD MBR signatures
2D0/A00	ALL	e820_map	E820 memory map table
				(array of struct e820entry)
D00/1EC	ALL	eddbuf		EDD data (array of struct edd_info)
