What:           /sys/devices/uncore_iio_x/dieX
Date:           February 2020
Contact:        Roman Sudarikov <roman.sudarikov@linux.intel.com>
Description:
                Each IIO stack (PCIe root port) has its own IIO PMON block, so
                each dieX file (where X is die number) holds "Segment:Root Bus"
                for PCIe root port, which can be monitored by that IIO PMON
                block.
                For example, on 4-die Xeon platform with up to 6 IIO stacks per
                die and, therefore, 6 IIO PMON blocks per die, the mapping of
                IIO PMON block 0 exposes as the following::

		    $ ls /sys/devices/uncore_iio_0/die*
		    -r--r--r-- /sys/devices/uncore_iio_0/die0
		    -r--r--r-- /sys/devices/uncore_iio_0/die1
		    -r--r--r-- /sys/devices/uncore_iio_0/die2
		    -r--r--r-- /sys/devices/uncore_iio_0/die3

		    $ tail /sys/devices/uncore_iio_0/die*
		    ==> /sys/devices/uncore_iio_0/die0 <==
		    0000:00
		    ==> /sys/devices/uncore_iio_0/die1 <==
		    0000:40
		    ==> /sys/devices/uncore_iio_0/die2 <==
		    0000:80
		    ==> /sys/devices/uncore_iio_0/die3 <==
		    0000:c0

                Which means::

		    IIO PMU 0 on die 0 belongs to PCI RP on bus 0x00, domain 0x0000
		    IIO PMU 0 on die 1 belongs to PCI RP on bus 0x40, domain 0x0000
		    IIO PMU 0 on die 2 belongs to PCI RP on bus 0x80, domain 0x0000
		    IIO PMU 0 on die 3 belongs to PCI RP on bus 0xc0, domain 0x0000
