Chinese translated version of Documentation/core-api/irq/index.rst

If you have any comment or update to the content, please contact the
original document maintainer directly.  However, if you have a problem
communicating in English you can also ask the Chinese maintainer for
help.  Contact the Chinese maintainer if this translation is outdated
or if there is a problem with the translation.

Maintainer: Eric W. Biederman <ebiederman@xmission.com>
Chinese maintainer: Fu Wei <tekkamanninja@gmail.com>
---------------------------------------------------------------------
Documentation/core-api/irq/index.rst 的中文翻译

如果想评论或更新本文的内容，请直接联系原文档的维护者。如果你使用英文
交流有困难的话，也可以向中文版维护者求助。如果本翻译更新不及时或者翻
译存在问题，请联系中文版维护者。
英文版维护者： Eric W. Biederman <ebiederman@xmission.com>
中文版维护者： 傅炜 Fu Wei <tekkamanninja@gmail.com>
中文版翻译者： 傅炜 Fu Wei <tekkamanninja@gmail.com>
中文版校译者： 傅炜 Fu Wei <tekkamanninja@gmail.com>


以下为正文
---------------------------------------------------------------------
何为 IRQ?

一个 IRQ 是来自某个设备的一个中断请求。目前，它们可以来自一个硬件引脚，
或来自一个数据包。多个设备可能连接到同个硬件引脚，从而共享一个 IRQ。

一个 IRQ 编号是用于告知硬件中断源的内核标识。通常情况下，这是一个
全局 irq_desc 数组的索引，但是除了在 linux/interrupt.h 中的实现，
具体的细节是体系结构特定的。

一个 IRQ 编号是设备上某个可能的中断源的枚举。通常情况下，枚举的编号是
该引脚在系统内中断控制器的所有输入引脚中的编号。对于 ISA 总线中的情况，
枚举的是在两个 i8259 中断控制器中 16 个输入引脚。

架构可以对 IRQ 编号指定额外的含义，在硬件涉及任何手工配置的情况下，
是被提倡的。ISA 的 IRQ 是一个分配这类额外含义的典型例子。
