NVIDIA Tegra210 timer

The Tegra210 timer provides fourteen 29-bit timer counters and one 32-bit
timestamp counter. The TMRs run at either a fixed 1 MHz clock rate derived
from the oscillator clock (TMR0-TMR9) or directly at the oscillator clock
(TMR10-TMR13). Each TMR can be programmed to generate one-shot, periodic,
or watchdog interrupts.

Required properties:
- compatible : "nvidia,tegra210-timer".
- reg : Specifies base physical address and size of the registers.
- interrupts : A list of 14 interrupts; one per each timer channels 0 through
  13.
- clocks : Must contain one entry, for the module clock.
  See ../clocks/clock-bindings.txt for details.

timer@60005000 {
	compatible = "nvidia,tegra210-timer";
	reg = <0x0 0x60005000 0x0 0x400>;
	interrupts = <GIC_SPI 156 IRQ_TYPE_LEVEL_HIGH>,
		     <GIC_SPI 0 IRQ_TYPE_LEVEL_HIGH>,
		     <GIC_SPI 1 IRQ_TYPE_LEVEL_HIGH>,
		     <GIC_SPI 41 IRQ_TYPE_LEVEL_HIGH>,
		     <GIC_SPI 42 IRQ_TYPE_LEVEL_HIGH>,
		     <GIC_SPI 121 IRQ_TYPE_LEVEL_HIGH>,
		     <GIC_SPI 152 IRQ_TYPE_LEVEL_HIGH>,
		     <GIC_SPI 153 IRQ_TYPE_LEVEL_HIGH>,
		     <GIC_SPI 154 IRQ_TYPE_LEVEL_HIGH>,
		     <GIC_SPI 155 IRQ_TYPE_LEVEL_HIGH>,
		     <GIC_SPI 176 IRQ_TYPE_LEVEL_HIGH>,
		     <GIC_SPI 177 IRQ_TYPE_LEVEL_HIGH>,
		     <GIC_SPI 178 IRQ_TYPE_LEVEL_HIGH>,
		     <GIC_SPI 179 IRQ_TYPE_LEVEL_HIGH>;
	clocks = <&tegra_car TEGRA210_CLK_TIMER>;
	clock-names = "timer";
};
