* Cadence MACB/GEM Ethernet controller

Required properties:
- compatible: Should be "cdns,[<chip>-]{macb|gem}"
  Use "cdns,at91rm9200-emac" Atmel at91rm9200 SoC.
  Use "cdns,at91sam9260-macb" for Atmel at91sam9 SoCs.
  Use "cdns,sam9x60-macb" for Microchip sam9x60 SoC.
  Use "cdns,np4-macb" for NP4 SoC devices.
  Use "cdns,at32ap7000-macb" for other 10/100 usage or use the generic form: "cdns,macb".
  Use "atmel,sama5d2-gem" for the GEM IP (10/100) available on Atmel sama5d2 SoCs.
  Use "atmel,sama5d3-macb" for the 10/100Mbit IP available on Atmel sama5d3 SoCs.
  Use "atmel,sama5d3-gem" for the Gigabit IP available on Atmel sama5d3 SoCs.
  Use "atmel,sama5d4-gem" for the GEM IP (10/100) available on Atmel sama5d4 SoCs.
  Use "cdns,zynq-gem" Xilinx Zynq-7xxx SoC.
  Use "cdns,zynqmp-gem" for Zynq Ultrascale+ MPSoC.
  Use "sifive,fu540-c000-gem" for SiFive FU540-C000 SoC.
  Use "microchip,sama7g5-emac" for Microchip SAMA7G5 ethernet interface.
  Use "microchip,sama7g5-gem" for Microchip SAMA7G5 gigabit ethernet interface.
  Or the generic form: "cdns,emac".
- reg: Address and length of the register set for the device
	For "sifive,fu540-c000-gem", second range is required to specify the
	address and length of the registers for GEMGXL Management block.
- interrupts: Should contain macb interrupt
- phy-mode: See ethernet.txt file in the same directory.
- clock-names: Tuple listing input clock names.
	Required elements: 'pclk', 'hclk'
	Optional elements: 'tx_clk'
	Optional elements: 'rx_clk' applies to cdns,zynqmp-gem
	Optional elements: 'tsu_clk'
- clocks: Phandles to input clocks.

The MAC address will be determined using the optional properties
defined in ethernet.txt.

Optional properties for PHY child node:
- reset-gpios : Should specify the gpio for phy reset
- magic-packet : If present, indicates that the hardware supports waking
  up via magic packet.
- phy-handle : see ethernet.txt file in the same directory

Examples:

	macb0: ethernet@fffc4000 {
		compatible = "cdns,at32ap7000-macb";
		reg = <0xfffc4000 0x4000>;
		interrupts = <21>;
		phy-mode = "rmii";
		local-mac-address = [3a 0e 03 04 05 06];
		clock-names = "pclk", "hclk", "tx_clk";
		clocks = <&clkc 30>, <&clkc 30>, <&clkc 13>;
		ethernet-phy@1 {
			reg = <0x1>;
			reset-gpios = <&pioE 6 1>;
		};
	};
