* Mediatek Media Data Path

Media Data Path is used for scaling and color space conversion.

Required properties (controller node):
- compatible: "mediatek,mt8173-mdp"
- mediatek,vpu: the node of video processor unit, see
  Documentation/devicetree/bindings/media/mediatek-vpu.txt for details.

Required properties (all function blocks, child node):
- compatible: Should be one of
        "mediatek,mt8173-mdp-rdma"  - read DMA
        "mediatek,mt8173-mdp-rsz"   - resizer
        "mediatek,mt8173-mdp-wdma"  - write DMA
        "mediatek,mt8173-mdp-wrot"  - write DMA with rotation
- reg: Physical base address and length of the function block register space
- clocks: device clocks, see
  Documentation/devicetree/bindings/clock/clock-bindings.txt for details.
- power-domains: a phandle to the power domain, see
  Documentation/devicetree/bindings/power/power_domain.txt for details.

Required properties (DMA function blocks, child node):
- compatible: Should be one of
        "mediatek,mt8173-mdp-rdma"
        "mediatek,mt8173-mdp-wdma"
        "mediatek,mt8173-mdp-wrot"
- iommus: should point to the respective IOMMU block with master port as
  argument, see Documentation/devicetree/bindings/iommu/mediatek,iommu.yaml
  for details.
- mediatek,larb: must contain the local arbiters in the current Socs, see
  Documentation/devicetree/bindings/memory-controllers/mediatek,smi-larb.yaml
  for details.

Example:
	mdp_rdma0: rdma@14001000 {
		compatible = "mediatek,mt8173-mdp-rdma";
			     "mediatek,mt8173-mdp";
		reg = <0 0x14001000 0 0x1000>;
		clocks = <&mmsys CLK_MM_MDP_RDMA0>,
			 <&mmsys CLK_MM_MUTEX_32K>;
		power-domains = <&scpsys MT8173_POWER_DOMAIN_MM>;
		iommus = <&iommu M4U_PORT_MDP_RDMA0>;
		mediatek,larb = <&larb0>;
		mediatek,vpu = <&vpu>;
	};

	mdp_rdma1: rdma@14002000 {
		compatible = "mediatek,mt8173-mdp-rdma";
		reg = <0 0x14002000 0 0x1000>;
		clocks = <&mmsys CLK_MM_MDP_RDMA1>,
			 <&mmsys CLK_MM_MUTEX_32K>;
		power-domains = <&scpsys MT8173_POWER_DOMAIN_MM>;
		iommus = <&iommu M4U_PORT_MDP_RDMA1>;
		mediatek,larb = <&larb4>;
	};

	mdp_rsz0: rsz@14003000 {
		compatible = "mediatek,mt8173-mdp-rsz";
		reg = <0 0x14003000 0 0x1000>;
		clocks = <&mmsys CLK_MM_MDP_RSZ0>;
		power-domains = <&scpsys MT8173_POWER_DOMAIN_MM>;
	};

	mdp_rsz1: rsz@14004000 {
		compatible = "mediatek,mt8173-mdp-rsz";
		reg = <0 0x14004000 0 0x1000>;
		clocks = <&mmsys CLK_MM_MDP_RSZ1>;
		power-domains = <&scpsys MT8173_POWER_DOMAIN_MM>;
	};

	mdp_rsz2: rsz@14005000 {
		compatible = "mediatek,mt8173-mdp-rsz";
		reg = <0 0x14005000 0 0x1000>;
		clocks = <&mmsys CLK_MM_MDP_RSZ2>;
		power-domains = <&scpsys MT8173_POWER_DOMAIN_MM>;
	};

	mdp_wdma0: wdma@14006000 {
		compatible = "mediatek,mt8173-mdp-wdma";
		reg = <0 0x14006000 0 0x1000>;
		clocks = <&mmsys CLK_MM_MDP_WDMA>;
		power-domains = <&scpsys MT8173_POWER_DOMAIN_MM>;
		iommus = <&iommu M4U_PORT_MDP_WDMA>;
		mediatek,larb = <&larb0>;
	};

	mdp_wrot0: wrot@14007000 {
		compatible = "mediatek,mt8173-mdp-wrot";
		reg = <0 0x14007000 0 0x1000>;
		clocks = <&mmsys CLK_MM_MDP_WROT0>;
		power-domains = <&scpsys MT8173_POWER_DOMAIN_MM>;
		iommus = <&iommu M4U_PORT_MDP_WROT0>;
		mediatek,larb = <&larb0>;
	};

	mdp_wrot1: wrot@14008000 {
		compatible = "mediatek,mt8173-mdp-wrot";
		reg = <0 0x14008000 0 0x1000>;
		clocks = <&mmsys CLK_MM_MDP_WROT1>;
		power-domains = <&scpsys MT8173_POWER_DOMAIN_MM>;
		iommus = <&iommu M4U_PORT_MDP_WROT1>;
		mediatek,larb = <&larb4>;
	};
