Properties for Jedec JC-42.4 compatible temperature sensors

Required properties:
- compatible: May include a device-specific string consisting of the
	      manufacturer and the name of the chip. A list of supported
	      chip names follows.
	      Must include "jedec,jc-42.4-temp" for any Jedec JC-42.4
	      compatible temperature sensor.

	      Supported chip names:
		adi,adt7408
		atmel,at30ts00
		atmel,at30tse004
		onnn,cat6095
		onnn,cat34ts02
		maxim,max6604
		microchip,mcp9804
		microchip,mcp9805
		microchip,mcp9808
		microchip,mcp98243
		microchip,mcp98244
		microchip,mcp9843
		nxp,se97
		nxp,se98
		st,stts2002
		st,stts2004
		st,stts3000
		st,stts424
		st,stts424e
		idt,tse2002
		idt,tse2004
		idt,ts3000
		idt,ts3001

- reg: I2C address

Optional properties:
- smbus-timeout-disable: When set, the smbus timeout function will be disabled.
			 This is not supported on all chips.

Example:

temp-sensor@1a {
	compatible = "jedec,jc-42.4-temp";
	reg = <0x1a>;
};
