Device tree configuration for Renesas IIC (sh_mobile) driver

Required properties:
- compatible      :
			- "renesas,iic-r8a73a4" (R-Mobile APE6)
			- "renesas,iic-r8a7740" (R-Mobile A1)
			- "renesas,iic-r8a7742" (RZ/G1H)
			- "renesas,iic-r8a7743" (RZ/G1M)
			- "renesas,iic-r8a7744" (RZ/G1N)
			- "renesas,iic-r8a7745" (RZ/G1E)
			- "renesas,iic-r8a774a1" (RZ/G2M)
			- "renesas,iic-r8a774b1" (RZ/G2N)
			- "renesas,iic-r8a774c0" (RZ/G2E)
			- "renesas,iic-r8a774e1" (RZ/G2H)
			- "renesas,iic-r8a7790" (R-Car H2)
			- "renesas,iic-r8a7791" (R-Car M2-W)
			- "renesas,iic-r8a7792" (R-Car V2H)
			- "renesas,iic-r8a7793" (R-Car M2-N)
			- "renesas,iic-r8a7794" (R-Car E2)
			- "renesas,iic-r8a7795" (R-Car H3)
			- "renesas,iic-r8a7796" (R-Car M3-W)
			- "renesas,iic-r8a77961" (R-Car M3-W+)
			- "renesas,iic-r8a77965" (R-Car M3-N)
			- "renesas,iic-r8a77990" (R-Car E3)
			- "renesas,iic-sh73a0" (SH-Mobile AG5)
			- "renesas,rcar-gen2-iic" (generic R-Car Gen2 or RZ/G1
							compatible device)
			- "renesas,rcar-gen3-iic" (generic R-Car Gen3 or RZ/G2
							compatible device)
			- "renesas,rmobile-iic" (generic device)

			When compatible with a generic R-Car version, nodes
			must list the SoC-specific version corresponding to
			the platform first followed by the generic R-Car
			version.

			When compatible with "renesas,rmobile-iic" it should
			be the last compatibility string listed.

			The r8a77990 (R-Car E3) and r8a774c0 (RZ/G2E)
			controllers are not considered compatible with
			"renesas,rcar-gen3-iic" or "renesas,rmobile-iic"
			due to the absence of automatic transmission registers.

- reg             : address start and address range size of device
- interrupts      : interrupt of device
- clocks          : clock for device
- #address-cells  : should be <1>
- #size-cells     : should be <0>

Optional properties:
- clock-frequency : frequency of bus clock in Hz. Default 100kHz if unset.
- dmas            : Must contain a list of two references to DMA
		    specifiers, one for transmission, and one for
		    reception.
- dma-names       : Must contain a list of two DMA names, "tx" and "rx".


Pinctrl properties might be needed, too. See there.

Example:

	iic0: i2c@e6500000 {
		compatible = "renesas,iic-r8a7790", "renesas,rcar-gen2-iic",
			     "renesas,rmobile-iic";
		reg = <0 0xe6500000 0 0x425>;
		interrupts = <0 174 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&mstp3_clks R8A7790_CLK_IIC0>;
		clock-frequency = <400000>;
		#address-cells = <1>;
		#size-cells = <0>;
	};
