What:		/sys/module/pch_phub/drivers/.../pch_mac
Date:		August 2010
KernelVersion:	2.6.35
Contact:	masa-korg@dsn.okisemi.com
Description:	Write/read GbE MAC address.

What:		/sys/module/pch_phub/drivers/.../pch_firmware
Date:		August 2010
KernelVersion:	2.6.35
Contact:	masa-korg@dsn.okisemi.com
Description:	Write/read Option ROM data.


What:		/sys/module/ehci_hcd/drivers/.../uframe_periodic_max
Date:		July 2011
KernelVersion:	3.1
Contact:	Kirill Smelkov <kirr@mns.spb.ru>
Description:	Maximum time allowed for periodic transfers per microframe (μs)

		[ USB 2.0 sets maximum allowed time for periodic transfers per
		  microframe to be 80%, that is 100 microseconds out of 125
		  microseconds (full microframe).

		  However there are cases, when 80% max isochronous bandwidth is
		  too limiting. For example two video streams could require 110
		  microseconds of isochronous bandwidth per microframe to work
		  together. ]

		Through this setting it is possible to raise the limit so that
		the host controller would allow allocating more than 100
		microseconds of periodic bandwidth per microframe.

		Beware, non-standard modes are usually not thoroughly tested by
		hardware designers, and the hardware can malfunction when this
		setting differ from default 100.

What:		/sys/module/*/{coresize,initsize}
Date:		Jan 2012
KernelVersion:»·3.3
Contact:	Kay Sievers <kay.sievers@vrfy.org>
Description:	Module size in bytes.

What:		/sys/module/*/taint
Date:		Jan 2012
KernelVersion:»·3.3
Contact:	Kay Sievers <kay.sievers@vrfy.org>
Description:	Module taint flags:
			P - proprietary module
			O - out-of-tree module
			F - force-loaded module
			C - staging driver module
