GPIO assisted NAND flash

The GPIO assisted NAND flash uses a memory mapped interface to
read/write the NAND commands and data and GPIO pins for the control
signals.

Required properties:
- compatible : "gpio-control-nand"
- reg : should specify localbus chip select and size used for the chip.  The
  resource describes the data bus connected to the NAND flash and all accesses
  are made in native endianness.
- #address-cells, #size-cells : Must be present if the device has sub-nodes
  representing partitions.
- gpios : specifies the gpio pins to control the NAND device.  nwp is an
  optional gpio and may be set to 0 if not present.

Optional properties:
- bank-width : Width (in bytes) of the device.  If not present, the width
  defaults to 1 byte.
- chip-delay : chip dependent delay for transferring data from array to
  read registers (tR).  If not present then a default of 20us is used.
- gpio-control-nand,io-sync-reg : A 64-bit physical address for a read
  location used to guard against bus reordering with regards to accesses to
  the GPIO's and the NAND flash data bus.  If present, then after changing
  GPIO state and before and after command byte writes, this register will be
  read to ensure that the GPIO accesses have completed.

Examples:

gpio-nand@1,0 {
	compatible = "gpio-control-nand";
	reg = <1 0x0000 0x2>;
	#address-cells = <1>;
	#size-cells = <1>;
	gpios = <&banka 1 0	/* rdy */
		 &banka 2 0 	/* nce */
		 &banka 3 0 	/* ale */
		 &banka 4 0 	/* cle */
		 0		/* nwp */>;

	partition@0 {
	...
	};
};
