.. SPDX-License-Identifier: GFDL-1.1-no-invariants-or-later
.. c:namespace:: V4L

.. _VIDIOC_G_EXT_CTRLS:

******************************************************************
ioctl VIDIOC_G_EXT_CTRLS, VIDIOC_S_EXT_CTRLS, VIDIOC_TRY_EXT_CTRLS
******************************************************************

Name
====

VIDIOC_G_EXT_CTRLS - VIDIOC_S_EXT_CTRLS - VIDIOC_TRY_EXT_CTRLS - Get or set the value of several controls, try control values

Synopsis
========

.. c:macro:: VIDIOC_G_EXT_CTRLS

``int ioctl(int fd, VIDIOC_G_EXT_CTRLS, struct v4l2_ext_controls *argp)``

.. c:macro:: VIDIOC_S_EXT_CTRLS

``int ioctl(int fd, VIDIOC_S_EXT_CTRLS, struct v4l2_ext_controls *argp)``

.. c:macro:: VIDIOC_TRY_EXT_CTRLS

``int ioctl(int fd, VIDIOC_TRY_EXT_CTRLS, struct v4l2_ext_controls *argp)``

Arguments
=========

``fd``
    File descriptor returned by :c:func:`open()`.

``argp``
    Pointer to struct :c:type:`v4l2_ext_controls`.

Description
===========

These ioctls allow the caller to get or set multiple controls
atomically. Control IDs are grouped into control classes (see
:ref:`ctrl-class`) and all controls in the control array must belong
to the same control class.

Applications must always fill in the ``count``, ``which``, ``controls``
and ``reserved`` fields of struct
:c:type:`v4l2_ext_controls`, and initialize the
struct :c:type:`v4l2_ext_control` array pointed to
by the ``controls`` fields.

To get the current value of a set of controls applications initialize
the ``id``, ``size`` and ``reserved2`` fields of each struct
:c:type:`v4l2_ext_control` and call the
:ref:`VIDIOC_G_EXT_CTRLS <VIDIOC_G_EXT_CTRLS>` ioctl. String controls must also set the
``string`` field. Controls of compound types
(``V4L2_CTRL_FLAG_HAS_PAYLOAD`` is set) must set the ``ptr`` field.

If the ``size`` is too small to receive the control result (only
relevant for pointer-type controls like strings), then the driver will
set ``size`` to a valid value and return an ``ENOSPC`` error code. You
should re-allocate the memory to this new size and try again. For the
string type it is possible that the same issue occurs again if the
string has grown in the meantime. It is recommended to call
:ref:`VIDIOC_QUERYCTRL` first and use
``maximum``\ +1 as the new ``size`` value. It is guaranteed that that is
sufficient memory.

N-dimensional arrays are set and retrieved row-by-row. You cannot set a
partial array, all elements have to be set or retrieved. The total size
is calculated as ``elems`` * ``elem_size``. These values can be obtained
by calling :ref:`VIDIOC_QUERY_EXT_CTRL <VIDIOC_QUERYCTRL>`.

To change the value of a set of controls applications initialize the
``id``, ``size``, ``reserved2`` and ``value/value64/string/ptr`` fields
of each struct :c:type:`v4l2_ext_control` and call
the :ref:`VIDIOC_S_EXT_CTRLS <VIDIOC_G_EXT_CTRLS>` ioctl. The controls will only be set if *all*
control values are valid.

To check if a set of controls have correct values applications
initialize the ``id``, ``size``, ``reserved2`` and
``value/value64/string/ptr`` fields of each struct
:c:type:`v4l2_ext_control` and call the
:ref:`VIDIOC_TRY_EXT_CTRLS <VIDIOC_G_EXT_CTRLS>` ioctl. It is up to the driver whether wrong
values are automatically adjusted to a valid value or if an error is
returned.

When the ``id`` or ``which`` is invalid drivers return an ``EINVAL`` error
code. When the value is out of bounds drivers can choose to take the
closest valid value or return an ``ERANGE`` error code, whatever seems more
appropriate. In the first case the new value is set in struct
:c:type:`v4l2_ext_control`. If the new control value
is inappropriate (e.g. the given menu index is not supported by the menu
control), then this will also result in an ``EINVAL`` error code error.

If ``request_fd`` is set to a not-yet-queued :ref:`request <media-request-api>`
file descriptor and ``which`` is set to ``V4L2_CTRL_WHICH_REQUEST_VAL``,
then the controls are not applied immediately when calling
:ref:`VIDIOC_S_EXT_CTRLS <VIDIOC_G_EXT_CTRLS>`, but instead are applied by
the driver for the buffer associated with the same request.
If the device does not support requests, then ``EACCES`` will be returned.
If requests are supported but an invalid request file descriptor is given,
then ``EINVAL`` will be returned.

An attempt to call :ref:`VIDIOC_S_EXT_CTRLS <VIDIOC_G_EXT_CTRLS>` for a
request that has already been queued will result in an ``EBUSY`` error.

If ``request_fd`` is specified and ``which`` is set to
``V4L2_CTRL_WHICH_REQUEST_VAL`` during a call to
:ref:`VIDIOC_G_EXT_CTRLS <VIDIOC_G_EXT_CTRLS>`, then it will return the
values of the controls at the time of request completion.
If the request is not yet completed, then this will result in an
``EACCES`` error.

The driver will only set/get these controls if all control values are
correct. This prevents the situation where only some of the controls
were set/get. Only low-level errors (e. g. a failed i2c command) can
still cause this situation.

.. tabularcolumns:: |p{6.8cm}|p{4.0cm}|p{6.5cm}|

.. c:type:: v4l2_ext_control

.. raw:: latex

   \footnotesize

.. cssclass:: longtable

.. flat-table:: struct v4l2_ext_control
    :header-rows:  0
    :stub-columns: 0
    :widths:       1 1 2

    * - __u32
      - ``id``
      - Identifies the control, set by the application.
    * - __u32
      - ``size``
      - The total size in bytes of the payload of this control.
    * - :cspan:`2` The ``size`` field is normally 0, but for pointer
	controls this should be set to the size of the memory that contains
	the payload or that will receive the payload.
	If :ref:`VIDIOC_G_EXT_CTRLS <VIDIOC_G_EXT_CTRLS>` finds that this value
	is less than is required to store the payload result, then it is set
	to a value large enough to store the payload result and ``ENOSPC`` is
	returned.

	.. note::

	   For string controls, this ``size`` field should
	   not be confused with the length of the string. This field refers
	   to the size of the memory that contains the string. The actual
	   *length* of the string may well be much smaller.
    * - __u32
      - ``reserved2``\ [1]
      - Reserved for future extensions. Drivers and applications must set
	the array to zero.
    * - union {
      - (anonymous)
    * - __s32
      - ``value``
      - New value or current value. Valid if this control is not of type
	``V4L2_CTRL_TYPE_INTEGER64`` and ``V4L2_CTRL_FLAG_HAS_PAYLOAD`` is
	not set.
    * - __s64
      - ``value64``
      - New value or current value. Valid if this control is of type
	``V4L2_CTRL_TYPE_INTEGER64`` and ``V4L2_CTRL_FLAG_HAS_PAYLOAD`` is
	not set.
    * - char *
      - ``string``
      - A pointer to a string. Valid if this control is of type
	``V4L2_CTRL_TYPE_STRING``.
    * - __u8 *
      - ``p_u8``
      - A pointer to a matrix control of unsigned 8-bit values. Valid if
	this control is of type ``V4L2_CTRL_TYPE_U8``.
    * - __u16 *
      - ``p_u16``
      - A pointer to a matrix control of unsigned 16-bit values. Valid if
	this control is of type ``V4L2_CTRL_TYPE_U16``.
    * - __u32 *
      - ``p_u32``
      - A pointer to a matrix control of unsigned 32-bit values. Valid if
	this control is of type ``V4L2_CTRL_TYPE_U32``.
    * - struct :c:type:`v4l2_area` *
      - ``p_area``
      - A pointer to a struct :c:type:`v4l2_area`. Valid if this control is
        of type ``V4L2_CTRL_TYPE_AREA``.
    * - struct :c:type:`v4l2_ctrl_h264_sps` *
      - ``p_h264_sps``
      - A pointer to a struct :c:type:`v4l2_ctrl_h264_sps`. Valid if this control is
        of type ``V4L2_CTRL_TYPE_H264_SPS``.
    * - struct :c:type:`v4l2_ctrl_h264_pps` *
      - ``p_h264_pps``
      - A pointer to a struct :c:type:`v4l2_ctrl_h264_pps`. Valid if this control is
        of type ``V4L2_CTRL_TYPE_H264_PPS``.
    * - struct :c:type:`v4l2_ctrl_h264_scaling_matrix` *
      - ``p_h264_scaling_matrix``
      - A pointer to a struct :c:type:`v4l2_ctrl_h264_scaling_matrix`. Valid if this control is
        of type ``V4L2_CTRL_TYPE_H264_SCALING_MATRIX``.
    * - struct :c:type:`v4l2_ctrl_h264_pred_weights` *
      - ``p_h264_pred_weights``
      - A pointer to a struct :c:type:`v4l2_ctrl_h264_pred_weights`. Valid if this control is
        of type ``V4L2_CTRL_TYPE_H264_PRED_WEIGHTS``.
    * - struct :c:type:`v4l2_ctrl_h264_slice_params` *
      - ``p_h264_slice_params``
      - A pointer to a struct :c:type:`v4l2_ctrl_h264_slice_params`. Valid if this control is
        of type ``V4L2_CTRL_TYPE_H264_SLICE_PARAMS``.
    * - struct :c:type:`v4l2_ctrl_h264_decode_params` *
      - ``p_h264_decode_params``
      - A pointer to a struct :c:type:`v4l2_ctrl_h264_decode_params`. Valid if this control is
        of type ``V4L2_CTRL_TYPE_H264_DECODE_PARAMS``.
    * - struct :c:type:`v4l2_ctrl_fwht_params` *
      - ``p_fwht_params``
      - A pointer to a struct :c:type:`v4l2_ctrl_fwht_params`. Valid if this control is
        of type ``V4L2_CTRL_TYPE_FWHT_PARAMS``.
    * - struct :c:type:`v4l2_ctrl_vp8_frame` *
      - ``p_vp8_frame``
      - A pointer to a struct :c:type:`v4l2_ctrl_vp8_frame`. Valid if this control is
        of type ``V4L2_CTRL_TYPE_VP8_FRAME``.
    * - struct :c:type:`v4l2_ctrl_mpeg2_sequence` *
      - ``p_mpeg2_sequence``
      - A pointer to a struct :c:type:`v4l2_ctrl_mpeg2_sequence`. Valid if this control is
        of type ``V4L2_CTRL_TYPE_MPEG2_SEQUENCE``.
    * - struct :c:type:`v4l2_ctrl_mpeg2_picture` *
      - ``p_mpeg2_picture``
      - A pointer to a struct :c:type:`v4l2_ctrl_mpeg2_picture`. Valid if this control is
        of type ``V4L2_CTRL_TYPE_MPEG2_PICTURE``.
    * - struct :c:type:`v4l2_ctrl_mpeg2_quantisation` *
      - ``p_mpeg2_quantisation``
      - A pointer to a struct :c:type:`v4l2_ctrl_mpeg2_quantisation`. Valid if this control is
        of type ``V4L2_CTRL_TYPE_MPEG2_QUANTISATION``.
    * - struct :c:type:`v4l2_ctrl_vp9_compressed_hdr` *
      - ``p_vp9_compressed_hdr_probs``
      - A pointer to a struct :c:type:`v4l2_ctrl_vp9_compressed_hdr`. Valid if this
        control is of type ``V4L2_CTRL_TYPE_VP9_COMPRESSED_HDR``.
    * - struct :c:type:`v4l2_ctrl_vp9_frame` *
      - ``p_vp9_frame``
      - A pointer to a struct :c:type:`v4l2_ctrl_vp9_frame`. Valid if this
        control is of type ``V4L2_CTRL_TYPE_VP9_FRAME``.
    * - struct :c:type:`v4l2_ctrl_hdr10_cll_info` *
      - ``p_hdr10_cll``
      - A pointer to a struct :c:type:`v4l2_ctrl_hdr10_cll_info`. Valid if this control is
        of type ``V4L2_CTRL_TYPE_HDR10_CLL_INFO``.
    * - struct :c:type:`v4l2_ctrl_hdr10_mastering_display` *
      - ``p_hdr10_mastering``
      - A pointer to a struct :c:type:`v4l2_ctrl_hdr10_mastering_display`. Valid if this control is
        of type ``V4L2_CTRL_TYPE_HDR10_MASTERING_DISPLAY``.
    * - struct :c:type:`v4l2_ctrl_hevc_sps` *
      - ``p_hevc_sps``
      - A pointer to a struct :c:type:`v4l2_ctrl_hevc_sps`. Valid if this
        control is of type ``V4L2_CTRL_TYPE_HEVC_SPS``.
    * - struct :c:type:`v4l2_ctrl_hevc_pps` *
      - ``p_hevc_pps``
      - A pointer to a struct :c:type:`v4l2_ctrl_hevc_pps`. Valid if this
        control is of type ``V4L2_CTRL_TYPE_HEVC_PPS``.
    * - struct :c:type:`v4l2_ctrl_hevc_slice_params` *
      - ``p_hevc_slice_params``
      - A pointer to a struct :c:type:`v4l2_ctrl_hevc_slice_params`. Valid if this
        control is of type ``V4L2_CTRL_TYPE_HEVC_SLICE_PARAMS``.
    * - struct :c:type:`v4l2_ctrl_hevc_scaling_matrix` *
      - ``p_hevc_scaling_matrix``
      - A pointer to a struct :c:type:`v4l2_ctrl_hevc_scaling_matrix`. Valid if this
        control is of type ``V4L2_CTRL_TYPE_HEVC_SCALING_MATRIX``.
    * - struct :c:type:`v4l2_ctrl_hevc_decode_params` *
      - ``p_hevc_decode_params``
      - A pointer to a struct :c:type:`v4l2_ctrl_hevc_decode_params`. Valid if this
        control is of type ``V4L2_CTRL_TYPE_HEVC_DECODE_PARAMS``.
    * - void *
      - ``ptr``
      - A pointer to a compound type which can be an N-dimensional array
	and/or a compound type (the control's type is >=
	``V4L2_CTRL_COMPOUND_TYPES``). Valid if
	``V4L2_CTRL_FLAG_HAS_PAYLOAD`` is set for this control.
    * - }
      -

.. raw:: latex

   \normalsize

.. tabularcolumns:: |p{4.0cm}|p{2.5cm}|p{10.8cm}|

.. c:type:: v4l2_ext_controls

.. cssclass:: longtable

.. flat-table:: struct v4l2_ext_controls
    :header-rows:  0
    :stub-columns: 0
    :widths:       1 1 2

    * - union {
      - (anonymous)
    * - __u32
      - ``which``
      - Which value of the control to get/set/try.
    * - :cspan:`2` ``V4L2_CTRL_WHICH_CUR_VAL`` will return the current value of
	the control, ``V4L2_CTRL_WHICH_DEF_VAL`` will return the default
	value of the control and ``V4L2_CTRL_WHICH_REQUEST_VAL`` indicates that
	these controls have to be retrieved from a request or tried/set for
	a request. In the latter case the ``request_fd`` field contains the
	file descriptor of the request that should be used. If the device
	does not support requests, then ``EACCES`` will be returned.

	When using ``V4L2_CTRL_WHICH_DEF_VAL`` be aware that you can only
	get the default value of the control, you cannot set or try it.

	For backwards compatibility you can also use a control class here
	(see :ref:`ctrl-class`). In that case all controls have to
	belong to that control class. This usage is deprecated, instead
	just use ``V4L2_CTRL_WHICH_CUR_VAL``. There are some very old
	drivers that do not yet support ``V4L2_CTRL_WHICH_CUR_VAL`` and
	that require a control class here. You can test for such drivers
	by setting ``which`` to ``V4L2_CTRL_WHICH_CUR_VAL`` and calling
	:ref:`VIDIOC_TRY_EXT_CTRLS <VIDIOC_G_EXT_CTRLS>` with a count of 0.
	If that fails, then the driver does not support ``V4L2_CTRL_WHICH_CUR_VAL``.
    * - __u32
      - ``ctrl_class``
      - Deprecated name kept for backwards compatibility. Use ``which`` instead.
    * - }
      -
    * - __u32
      - ``count``
      - The number of controls in the controls array. May also be zero.
    * - __u32
      - ``error_idx``
      - Index of the failing control. Set by the driver in case of an error.
    * - :cspan:`2` If the error is associated
	with a particular control, then ``error_idx`` is set to the index
	of that control. If the error is not related to a specific
	control, or the validation step failed (see below), then
	``error_idx`` is set to ``count``. The value is undefined if the
	ioctl returned 0 (success).

	Before controls are read from/written to hardware a validation
	step takes place: this checks if all controls in the list are
	valid controls, if no attempt is made to write to a read-only
	control or read from a write-only control, and any other up-front
	checks that can be done without accessing the hardware. The exact
	validations done during this step are driver dependent since some
	checks might require hardware access for some devices, thus making
	it impossible to do those checks up-front. However, drivers should
	make a best-effort to do as many up-front checks as possible.

	This check is done to avoid leaving the hardware in an
	inconsistent state due to easy-to-avoid problems. But it leads to
	another problem: the application needs to know whether an error
	came from the validation step (meaning that the hardware was not
	touched) or from an error during the actual reading from/writing
	to hardware.

	The, in hindsight quite poor, solution for that is to set
	``error_idx`` to ``count`` if the validation failed. This has the
	unfortunate side-effect that it is not possible to see which
	control failed the validation. If the validation was successful
	and the error happened while accessing the hardware, then
	``error_idx`` is less than ``count`` and only the controls up to
	``error_idx-1`` were read or written correctly, and the state of
	the remaining controls is undefined.

	Since :ref:`VIDIOC_TRY_EXT_CTRLS <VIDIOC_G_EXT_CTRLS>` does not access hardware there is
	also no need to handle the validation step in this special way, so
	``error_idx`` will just be set to the control that failed the
	validation step instead of to ``count``. This means that if
	:ref:`VIDIOC_S_EXT_CTRLS <VIDIOC_G_EXT_CTRLS>` fails with ``error_idx`` set to ``count``,
	then you can call :ref:`VIDIOC_TRY_EXT_CTRLS <VIDIOC_G_EXT_CTRLS>` to try to discover the
	actual control that failed the validation step. Unfortunately,
	there is no ``TRY`` equivalent for :ref:`VIDIOC_G_EXT_CTRLS <VIDIOC_G_EXT_CTRLS>`.
    * - __s32
      - ``request_fd``
      - File descriptor of the request to be used by this operation. Only
	valid if ``which`` is set to ``V4L2_CTRL_WHICH_REQUEST_VAL``.
	If the device does not support requests, then ``EACCES`` will be returned.
	If requests are supported but an invalid request file descriptor is
	given, then ``EINVAL`` will be returned.
    * - __u32
      - ``reserved``\ [1]
      - Reserved for future extensions.

	Drivers and applications must set the array to zero.
    * - struct :c:type:`v4l2_ext_control` *
      - ``controls``
      - Pointer to an array of ``count`` v4l2_ext_control structures.

	Ignored if ``count`` equals zero.

.. tabularcolumns:: |p{7.3cm}|p{2.0cm}|p{8.0cm}|

.. cssclass:: longtable

.. _ctrl-class:

.. flat-table:: Control classes
    :header-rows:  0
    :stub-columns: 0
    :widths:       3 1 4

    * - ``V4L2_CTRL_CLASS_USER``
      - 0x980000
      - The class containing user controls. These controls are described
	in :ref:`control`. All controls that can be set using the
	:ref:`VIDIOC_S_CTRL <VIDIOC_G_CTRL>` and
	:ref:`VIDIOC_G_CTRL <VIDIOC_G_CTRL>` ioctl belong to this
	class.
    * - ``V4L2_CTRL_CLASS_CODEC``
      - 0x990000
      - The class containing stateful codec controls. These controls are
	described in :ref:`codec-controls`.
    * - ``V4L2_CTRL_CLASS_CAMERA``
      - 0x9a0000
      - The class containing camera controls. These controls are described
	in :ref:`camera-controls`.
    * - ``V4L2_CTRL_CLASS_FM_TX``
      - 0x9b0000
      - The class containing FM Transmitter (FM TX) controls. These
	controls are described in :ref:`fm-tx-controls`.
    * - ``V4L2_CTRL_CLASS_FLASH``
      - 0x9c0000
      - The class containing flash device controls. These controls are
	described in :ref:`flash-controls`.
    * - ``V4L2_CTRL_CLASS_JPEG``
      - 0x9d0000
      - The class containing JPEG compression controls. These controls are
	described in :ref:`jpeg-controls`.
    * - ``V4L2_CTRL_CLASS_IMAGE_SOURCE``
      - 0x9e0000
      - The class containing image source controls. These controls are
	described in :ref:`image-source-controls`.
    * - ``V4L2_CTRL_CLASS_IMAGE_PROC``
      - 0x9f0000
      - The class containing image processing controls. These controls are
	described in :ref:`image-process-controls`.
    * - ``V4L2_CTRL_CLASS_FM_RX``
      - 0xa10000
      - The class containing FM Receiver (FM RX) controls. These controls
	are described in :ref:`fm-rx-controls`.
    * - ``V4L2_CTRL_CLASS_RF_TUNER``
      - 0xa20000
      - The class containing RF tuner controls. These controls are
	described in :ref:`rf-tuner-controls`.
    * - ``V4L2_CTRL_CLASS_DETECT``
      - 0xa30000
      - The class containing motion or object detection controls. These controls
        are described in :ref:`detect-controls`.
    * - ``V4L2_CTRL_CLASS_CODEC_STATELESS``
      - 0xa40000
      - The class containing stateless codec controls. These controls are
	described in :ref:`codec-stateless-controls`.
    * - ``V4L2_CTRL_CLASS_COLORIMETRY``
      - 0xa50000
      - The class containing colorimetry controls. These controls are
	described in :ref:`colorimetry-controls`.

Return Value
============

On success 0 is returned, on error -1 and the ``errno`` variable is set
appropriately. The generic error codes are described at the
:ref:`Generic Error Codes <gen-errors>` chapter.

EINVAL
    The struct :c:type:`v4l2_ext_control` ``id`` is
    invalid, or the struct :c:type:`v4l2_ext_controls`
    ``which`` is invalid, or the struct
    :c:type:`v4l2_ext_control` ``value`` was
    inappropriate (e.g. the given menu index is not supported by the
    driver), or the ``which`` field was set to ``V4L2_CTRL_WHICH_REQUEST_VAL``
    but the given ``request_fd`` was invalid or ``V4L2_CTRL_WHICH_REQUEST_VAL``
    is not supported by the kernel.
    This error code is also returned by the
    :ref:`VIDIOC_S_EXT_CTRLS <VIDIOC_G_EXT_CTRLS>` and :ref:`VIDIOC_TRY_EXT_CTRLS <VIDIOC_G_EXT_CTRLS>` ioctls if two or
    more control values are in conflict.

ERANGE
    The struct :c:type:`v4l2_ext_control` ``value``
    is out of bounds.

EBUSY
    The control is temporarily not changeable, possibly because another
    applications took over control of the device function this control
    belongs to, or (if the ``which`` field was set to
    ``V4L2_CTRL_WHICH_REQUEST_VAL``) the request was queued but not yet
    completed.

ENOSPC
    The space reserved for the control's payload is insufficient. The
    field ``size`` is set to a value that is enough to store the payload
    and this error code is returned.

EACCES
    Attempt to try or set a read-only control, or to get a write-only
    control, or to get a control from a request that has not yet been
    completed.

    Or the ``which`` field was set to ``V4L2_CTRL_WHICH_REQUEST_VAL`` but the
    device does not support requests.

    Or if there is an attempt to set an inactive control and the driver is
    not capable of caching the new value until the control is active again.
