Rockchip specific extensions to the Synopsys Designware MIPI DSI
================================

Required properties:
- #address-cells: Should be <1>.
- #size-cells: Should be <0>.
- compatible: one of
	"rockchip,px30-mipi-dsi", "snps,dw-mipi-dsi"
	"rockchip,rk3288-mipi-dsi", "snps,dw-mipi-dsi"
	"rockchip,rk3399-mipi-dsi", "snps,dw-mipi-dsi"
	"rockchip,rk3568-mipi-dsi", "snps,dw-mipi-dsi"
- reg: Represent the physical address range of the controller.
- interrupts: Represent the controller's interrupt to the CPU(s).
- clocks, clock-names: Phandles to the controller's pll reference
  clock(ref) when using an internal dphy and APB clock(pclk).
  For RK3399, a phy config clock (phy_cfg) and a grf clock(grf)
  are required. As described in [1].
- rockchip,grf: this soc should set GRF regs to mux vopl/vopb.
- ports: contain a port node with endpoint definitions as defined in [2].
  For vopb,set the reg = <0> and set the reg = <1> for vopl.
- video port 0 for the VOP input, the remote endpoint maybe vopb or vopl
- video port 1 for either a panel or subsequent encoder

Optional properties:
- phys: from general PHY binding: the phandle for the PHY device.
- phy-names: Should be "dphy" if phys references an external phy.
- #phy-cells: Defined when used as ISP phy, should be 0.
- power-domains: a phandle to mipi dsi power domain node.
- resets: list of phandle + reset specifier pairs, as described in [3].
- reset-names: string reset name, must be "apb".

[1] Documentation/devicetree/bindings/clock/clock-bindings.txt
[2] Documentation/devicetree/bindings/media/video-interfaces.txt
[3] Documentation/devicetree/bindings/reset/reset.txt

Example:
	mipi_dsi: mipi@ff960000 {
		#address-cells = <1>;
		#size-cells = <0>;
		compatible = "rockchip,rk3288-mipi-dsi", "snps,dw-mipi-dsi";
		reg = <0xff960000 0x4000>;
		interrupts = <GIC_SPI 83 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&cru SCLK_MIPI_24M>, <&cru PCLK_MIPI_DSI0>;
		clock-names = "ref", "pclk";
		resets = <&cru SRST_MIPIDSI0>;
		reset-names = "apb";
		rockchip,grf = <&grf>;

		ports {
			#address-cells = <1>;
			#size-cells = <0>;

			mipi_in: port@0 {
				reg = <0>;
				#address-cells = <1>;
				#size-cells = <0>;

				mipi_in_vopb: endpoint@0 {
					reg = <0>;
					remote-endpoint = <&vopb_out_mipi>;
				};
				mipi_in_vopl: endpoint@1 {
					reg = <1>;
					remote-endpoint = <&vopl_out_mipi>;
				};
			};

			mipi_out: port@1 {
				reg = <1>;
				#address-cells = <1>;
				#size-cells = <0>;

				mipi_out_panel: endpoint {
					remote-endpoint = <&panel_in_mipi>;
				};
			};
		};

		panel {
			compatible ="boe,tv080wum-nl0";
			reg = <0>;

			enable-gpios = <&gpio7 3 GPIO_ACTIVE_HIGH>;
			pinctrl-names = "default";
			pinctrl-0 = <&lcd_en>;
			backlight = <&backlight>;

			port {
				panel_in_mipi: endpoint {
					remote-endpoint = <&mipi_out_panel>;
				};
			};
		};
	};
