.. SPDX-License-Identifier: GPL-2.0

==================================================
Collaborative Processor Performance Control (CPPC)
==================================================

.. _cppc_sysfs:

CPPC
====

CPPC defined in the ACPI spec describes a mechanism for the OS to manage the
performance of a logical processor on a contiguous and abstract performance
scale. CPPC exposes a set of registers to describe abstract performance scale,
to request performance levels and to measure per-cpu delivered performance.

For more details on CPPC please refer to the ACPI specification at:

http://uefi.org/specifications

Some of the CPPC registers are exposed via sysfs under::

  /sys/devices/system/cpu/cpuX/acpi_cppc/

for each cpu X::

  $ ls -lR  /sys/devices/system/cpu/cpu0/acpi_cppc/
  /sys/devices/system/cpu/cpu0/acpi_cppc/:
  total 0
  -r--r--r-- 1 root root 65536 Mar  5 19:38 feedback_ctrs
  -r--r--r-- 1 root root 65536 Mar  5 19:38 highest_perf
  -r--r--r-- 1 root root 65536 Mar  5 19:38 lowest_freq
  -r--r--r-- 1 root root 65536 Mar  5 19:38 lowest_nonlinear_perf
  -r--r--r-- 1 root root 65536 Mar  5 19:38 lowest_perf
  -r--r--r-- 1 root root 65536 Mar  5 19:38 nominal_freq
  -r--r--r-- 1 root root 65536 Mar  5 19:38 nominal_perf
  -r--r--r-- 1 root root 65536 Mar  5 19:38 reference_perf
  -r--r--r-- 1 root root 65536 Mar  5 19:38 wraparound_time

* highest_perf : Highest performance of this processor (abstract scale).
* nominal_perf : Highest sustained performance of this processor
  (abstract scale).
* lowest_nonlinear_perf : Lowest performance of this processor with nonlinear
  power savings (abstract scale).
* lowest_perf : Lowest performance of this processor (abstract scale).

* lowest_freq : CPU frequency corresponding to lowest_perf (in MHz).
* nominal_freq : CPU frequency corresponding to nominal_perf (in MHz).
  The above frequencies should only be used to report processor performance in
  frequency instead of abstract scale. These values should not be used for any
  functional decisions.

* feedback_ctrs : Includes both Reference and delivered performance counter.
  Reference counter ticks up proportional to processor's reference performance.
  Delivered counter ticks up proportional to processor's delivered performance.
* wraparound_time: Minimum time for the feedback counters to wraparound
  (seconds).
* reference_perf : Performance level at which reference performance counter
  accumulates (abstract scale).


Computing Average Delivered Performance
=======================================

Below describes the steps to compute the average performance delivered by
taking two different snapshots of feedback counters at time T1 and T2.

  T1: Read feedback_ctrs as fbc_t1
      Wait or run some workload

  T2: Read feedback_ctrs as fbc_t2

::

  delivered_counter_delta = fbc_t2[del] - fbc_t1[del]
  reference_counter_delta = fbc_t2[ref] - fbc_t1[ref]

  delivered_perf = (refernce_perf x delivered_counter_delta) / reference_counter_delta
