Kernel driver ibmaem
======================

Supported systems:
  * Any recent IBM System X server with Active Energy Manager support.
    This includes the x3350, x3550, x3650, x3655, x3755, x3850 M2,
    x3950 M2, and certain HS2x/LS2x/QS2x blades.  The IPMI host interface
    driver ("ipmi-si") needs to be loaded for this driver to do anything.
    Prefix: 'ibmaem'
    Datasheet: Not available

Author: Darrick J. Wong

Description
-----------

This driver implements sensor reading support for the energy and power
meters available on various IBM System X hardware through the BMC.  All
sensor banks will be exported as platform devices; this driver can talk
to both v1 and v2 interfaces.  This driver is completely separate from the
older ibmpex driver.

The v1 AEM interface has a simple set of features to monitor energy use.
There is a register that displays an estimate of raw energy consumption
since the last BMC reset, and a power sensor that returns average power
use over a configurable interval.

The v2 AEM interface is a bit more sophisticated, being able to present
a wider range of energy and power use registers, the power cap as
set by the AEM software, and temperature sensors.

Special Features
----------------

The "power_cap" value displays the current system power cap, as set by
the Active Energy Manager software.  Setting the power cap from the host
is not currently supported.
