*Device-Tree bindings for ST SW reset functionality

Required properties:
- compatible: should be "st,<chip>-restart".
- st,syscfg: should be a phandle of the syscfg node.

Example node:
	restart {
		compatible = "st,stih416-restart";
		st,syscfg = <&syscfg_sbc>;
	};
