GMT G762/G763 PWM Fan controller

Required node properties:

 - "compatible": must be either "gmt,g762" or "gmt,g763"
 - "reg": I2C bus address of the device
 - "clocks": a fixed clock providing input clock frequency
	     on CLK pin of the chip.

Optional properties:

 - "fan_startv": fan startup voltage. Accepted values are 0, 1, 2 and 3.
	       The higher the more.

 - "pwm_polarity": pwm polarity. Accepted values are 0 (positive duty)
	       and 1 (negative duty).

 - "fan_gear_mode": fan gear mode. Supported values are 0, 1 and 2.

If an optional property is not set in .dts file, then current value is kept
unmodified (e.g. u-boot installed value).

Additional information on operational parameters for the device is available
in Documentation/hwmon/g762. A detailed datasheet for the device is available
at http://natisbad.org/NAS/refs/GMT_EDS-762_763-080710-0.2.pdf.

Example g762 node:

   clocks {
	#address-cells = <1>;
	#size-cells = <0>;

	g762_clk: fixedclk {
		 compatible = "fixed-clock";
		 #clock-cells = <0>;
		 clock-frequency = <8192>;
	}
   }

   g762: g762@3e {
	compatible = "gmt,g762";
	reg = <0x3e>;
	clocks = <&g762_clk>
	fan_gear_mode = <0>; /* chip default */
	fan_startv = <1>;    /* chip default */
	pwm_polarity = <0>;  /* chip default */
   };
