Broadcom BCM4708 device tree bindings
-------------------------------------------

Boards with the BCM4708 SoC shall have the following properties:

Required root node property:

compatible = "brcm,bcm4708";
