<refentry id="FE_DISEQC_RESET_OVERLOAD">
  <refmeta>
    <refentrytitle>ioctl FE_DISEQC_RESET_OVERLOAD</refentrytitle>
    &manvol;
  </refmeta>

  <refnamediv>
    <refname>FE_DISEQC_RESET_OVERLOAD</refname>
    <refpurpose>Restores the power to the antenna subsystem, if it was powered
	off due to power overload.</refpurpose>
  </refnamediv>

  <refsynopsisdiv>
    <funcsynopsis>
      <funcprototype>
	<funcdef>int <function>ioctl</function></funcdef>
	<paramdef>int <parameter>fd</parameter></paramdef>
	<paramdef>int <parameter>request</parameter></paramdef>
	<paramdef>NULL</paramdef>
      </funcprototype>
    </funcsynopsis>
  </refsynopsisdiv>

  <refsect1>
    <title>Arguments</title>
        <variablelist>
      <varlistentry>
	<term><parameter>fd</parameter></term>
	<listitem>
	  <para>&fe_fd;</para>
	</listitem>
      </varlistentry>
      <varlistentry>
	<term><parameter>request</parameter></term>
	<listitem>
	  <para>FE_DISEQC_RESET_OVERLOAD</para>
	</listitem>
      </varlistentry>
    </variablelist>
  </refsect1>

  <refsect1>
    <title>Description</title>

    <para>If the bus has been automatically powered off due to power overload, this ioctl
 call restores the power to the bus. The call requires read/write access to the
 device. This call has no effect if the device is manually powered off. Not all
 DVB adapters support this ioctl.</para>
&return-value-dvb;
</refsect1>
</refentry>
