RK808 Power Management Integrated Circuit

Required properties:
- compatible: "rockchip,rk808"
- reg: I2C slave address
- interrupt-parent: The parent interrupt controller.
- interrupts: the interrupt outputs of the controller.
- #clock-cells: from common clock binding; shall be set to 1 (multiple clock
  outputs). See <dt-bindings/clock/rockchip,rk808.h> for clock IDs.

Optional properties:
- clock-output-names: From common clock binding to override the
  default output clock name
- rockchip,system-power-controller: Telling whether or not this pmic is controlling
  the system power.
- vcc1-supply:  The input supply for DCDC_REG1
- vcc2-supply:  The input supply for DCDC_REG2
- vcc3-supply:  The input supply for DCDC_REG3
- vcc4-supply:  The input supply for DCDC_REG4
- vcc6-supply:  The input supply for LDO_REG1 and LDO_REG2
- vcc7-supply:  The input supply for LDO_REG3 and LDO_REG7
- vcc8-supply:  The input supply for SWITCH_REG1
- vcc9-supply:  The input supply for LDO_REG4 and LDO_REG5
- vcc10-supply: The input supply for LDO_REG6
- vcc11-supply: The input supply for LDO_REG8
- vcc12-supply: The input supply for SWITCH_REG2

Regulators: All the regulators of RK808 to be instantiated shall be
listed in a child node named 'regulators'. Each regulator is represented
by a child node of the 'regulators' node.

	regulator-name {
		/* standard regulator bindings here */
	};

Following regulators of the RK808 PMIC block are supported. Note that
the 'n' in regulator name, as in DCDC_REGn or LDOn, represents the DCDC or LDO
number as described in RK808 datasheet.

	- DCDC_REGn
		- valid values for n are 1 to 4.
	- LDO_REGn
		- valid values for n are 1 to 8.
	- SWITCH_REGn
		- valid values for n are 1 to 2

Standard regulator bindings are used inside regulator subnodes. Check
  Documentation/devicetree/bindings/regulator/regulator.txt
for more details

Example:
	rk808: pmic@1b {
		compatible = "rockchip,rk808";
		clock-output-names = "xin32k", "rk808-clkout2";
		interrupt-parent = <&gpio0>;
		interrupts = <4 IRQ_TYPE_LEVEL_LOW>;
		pinctrl-names = "default";
		pinctrl-0 = <&pmic_int>;
		reg = <0x1b>;
		rockchip,system-power-controller;
		wakeup-source;
		#clock-cells = <1>;

		vcc8-supply = <&vcc_18>;
		vcc9-supply = <&vcc_io>;
		vcc10-supply = <&vcc_io>;
		vcc12-supply = <&vcc_io>;
		vddio-supply = <&vccio_pmu>;

		regulators {
			vdd_cpu: DCDC_REG1 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <750000>;
				regulator-max-microvolt = <1300000>;
				regulator-name = "vdd_arm";
			};

			vdd_gpu: DCDC_REG2 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <850000>;
				regulator-max-microvolt = <1250000>;
				regulator-name = "vdd_gpu";
			};

			vcc_ddr: DCDC_REG3 {
				regulator-always-on;
				regulator-boot-on;
				regulator-name = "vcc_ddr";
			};

			vcc_io: DCDC_REG4 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <3300000>;
				regulator-max-microvolt = <3300000>;
				regulator-name = "vcc_io";
			};

			vccio_pmu: LDO_REG1 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <3300000>;
				regulator-max-microvolt = <3300000>;
				regulator-name = "vccio_pmu";
			};

			vcc_tp: LDO_REG2 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <3300000>;
				regulator-max-microvolt = <3300000>;
				regulator-name = "vcc_tp";
			};

			vdd_10: LDO_REG3 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1000000>;
				regulator-max-microvolt = <1000000>;
				regulator-name = "vdd_10";
			};

			vcc18_lcd: LDO_REG4 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
				regulator-name = "vcc18_lcd";
			};

			vccio_sd: LDO_REG5 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <3300000>;
				regulator-name = "vccio_sd";
			};

			vdd10_lcd: LDO_REG6 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1000000>;
				regulator-max-microvolt = <1000000>;
				regulator-name = "vdd10_lcd";
			};

			vcc_18: LDO_REG7 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
				regulator-name = "vcc_18";
			};

			vcca_codec: LDO_REG8 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <3300000>;
				regulator-max-microvolt = <3300000>;
				regulator-name = "vcca_codec";
			};

			vcc_wl: SWITCH_REG1 {
				regulator-always-on;
				regulator-boot-on;
				regulator-name = "vcc_wl";
			};

			vcc_lcd: SWITCH_REG2 {
				regulator-always-on;
				regulator-boot-on;
				regulator-name = "vcc_lcd";
			};
		};
	};
