* Samsung Image Rotator

Required properties:
  - compatible : value should be one of the following:
	(a) "samsung,exynos4210-rotator" for Rotator IP in Exynos4210
	(b) "samsung,exynos4212-rotator" for Rotator IP in Exynos4212/4412
	(c) "samsung,exynos5250-rotator" for Rotator IP in Exynos5250

  - reg : Physical base address of the IP registers and length of memory
	  mapped region.

  - interrupts : Interrupt specifier for rotator interrupt, according to format
		 specific to interrupt parent.

  - clocks : Clock specifier for rotator clock, according to generic clock
	     bindings. (See Documentation/devicetree/bindings/clock/exynos*.txt)

  - clock-names : Names of clocks. For exynos rotator, it should be "rotator".

Example:
	rotator@12810000 {
		compatible = "samsung,exynos4210-rotator";
		reg = <0x12810000 0x1000>;
		interrupts = <0 83 0>;
		clocks = <&clock 278>;
		clock-names = "rotator";
	};
