Renesas H8S2678 PLL clock

This device is Clock multiplyer

Required Properties:

  - compatible: Must be "renesas,h8s2678-pll-clock"

  - clocks: Reference to the parent clocks

  - #clock-cells: Must be 0

  - reg: Two rate selector (Multiply / Divide) register address

Example
-------

		pllclk: pllclk {
			compatible = "renesas,h8s2678-pll-clock";
			clocks = <&xclk>;
			#clock-cells = <0>;
			reg = <0xfee03b 2>, <0xfee045 2>;
		};
