Qualcomm adreno/snapdragon hdmi output

Required properties:
- compatible: one of the following
   * "qcom,hdmi-tx-8994"
   * "qcom,hdmi-tx-8084"
   * "qcom,hdmi-tx-8974"
   * "qcom,hdmi-tx-8660"
   * "qcom,hdmi-tx-8960"
- reg: Physical base address and length of the controller's registers
- reg-names: "core_physical"
- interrupts: The interrupt signal from the hdmi block.
- clocks: device clocks
  See ../clocks/clock-bindings.txt for details.
- qcom,hdmi-tx-ddc-clk-gpio: ddc clk pin
- qcom,hdmi-tx-ddc-data-gpio: ddc data pin
- qcom,hdmi-tx-hpd-gpio: hpd pin
- core-vdda-supply: phandle to supply regulator
- hdmi-mux-supply: phandle to mux regulator

Optional properties:
- qcom,hdmi-tx-mux-en-gpio: hdmi mux enable pin
- qcom,hdmi-tx-mux-sel-gpio: hdmi mux select pin
- pinctrl-names: the pin control state names; should contain "default"
- pinctrl-0: the default pinctrl state (active)
- pinctrl-1: the "sleep" pinctrl state

Example:

/ {
	...

	hdmi: qcom,hdmi-tx-8960@4a00000 {
		compatible = "qcom,hdmi-tx-8960";
		reg-names = "core_physical";
		reg = <0x04a00000 0x1000>;
		interrupts = <GIC_SPI 79 0>;
		clock-names =
		    "core_clk",
		    "master_iface_clk",
		    "slave_iface_clk";
		clocks =
		    <&mmcc HDMI_APP_CLK>,
		    <&mmcc HDMI_M_AHB_CLK>,
		    <&mmcc HDMI_S_AHB_CLK>;
		qcom,hdmi-tx-ddc-clk = <&msmgpio 70 GPIO_ACTIVE_HIGH>;
		qcom,hdmi-tx-ddc-data = <&msmgpio 71 GPIO_ACTIVE_HIGH>;
		qcom,hdmi-tx-hpd = <&msmgpio 72 GPIO_ACTIVE_HIGH>;
		core-vdda-supply = <&pm8921_hdmi_mvs>;
		hdmi-mux-supply = <&ext_3p3v>;
		pinctrl-names = "default", "sleep";
		pinctrl-0 = <&hpd_active  &ddc_active  &cec_active>;
		pinctrl-1 = <&hpd_suspend &ddc_suspend &cec_suspend>;
	};
};
