Freescale L2 Cache Controller

L2 cache is present in Freescale's QorIQ and QorIQ Qonverge platforms.
The cache bindings explained below are ePAPR compliant

Required Properties:

- compatible	: Should include "fsl,chip-l2-cache-controller" and "cache"
		  where chip is the processor (bsc9132, npc8572 etc.)
- reg		: Address and size of L2 cache controller registers
- cache-size	: Size of the entire L2 cache
- interrupts	: Error interrupt of L2 controller
- cache-line-size : Size of L2 cache lines

Example:

	L2: l2-cache-controller@20000 {
		compatible = "fsl,bsc9132-l2-cache-controller", "cache";
		reg = <0x20000 0x1000>;
		cache-line-size = <32>; // 32 bytes
		cache-size = <0x40000>; // L2,256K
		interrupts = <16 2 1 0>;
	};
