Broadcom Cygnus GPIO/PINCONF Controller

Required properties:

- compatible:
    Must be "brcm,cygnus-ccm-gpio", "brcm,cygnus-asiu-gpio", or
    "brcm,cygnus-crmu-gpio"

- reg:
    Define the base and range of the I/O address space that contains the Cygnus
GPIO/PINCONF controller registers

- #gpio-cells:
    Must be two. The first cell is the GPIO pin number (within the
controller's pin space) and the second cell is used for the following:
    bit[0]: polarity (0 for active high and 1 for active low)

- gpio-controller:
    Specifies that the node is a GPIO controller

Optional properties:

- interrupts:
    Interrupt ID

- interrupt-controller:
    Specifies that the node is an interrupt controller

- pinmux:
    Specifies the phandle to the IOMUX device, where pins can be individually
muxed to GPIO

Supported generic PINCONF properties in child nodes:

- pins:
    The list of pins (within the controller's own pin space) that properties
in the node apply to. Pin names are "gpio-<pin>"

- bias-disable:
    Disable pin bias

- bias-pull-up:
    Enable internal pull up resistor

- bias-pull-down:
    Enable internal pull down resistor

- drive-strength:
    Valid drive strength values include 2, 4, 6, 8, 10, 12, 14, 16 (mA)

Example:
	gpio_ccm: gpio@1800a000 {
		compatible = "brcm,cygnus-ccm-gpio";
		reg = <0x1800a000 0x50>,
		      <0x0301d164 0x20>;
		#gpio-cells = <2>;
		gpio-controller;
		interrupts = <GIC_SPI 84 IRQ_TYPE_LEVEL_HIGH>;
		interrupt-controller;

		touch_pins: touch_pins {
			pwr: pwr {
				pins = "gpio-0";
				drive-strength = <16>;
			};

			event: event {
				pins = "gpio-1";
				bias-pull-up;
			};
		};
	};

	gpio_asiu: gpio@180a5000 {
		compatible = "brcm,cygnus-asiu-gpio";
		reg = <0x180a5000 0x668>;
		#gpio-cells = <2>;
		gpio-controller;
		interrupts = <GIC_SPI 174 IRQ_TYPE_LEVEL_HIGH>;
		interrupt-controller;
	};

	/*
	 * Touchscreen that uses the CCM GPIO 0 and 1
	 */
	tsc {
		...
		...
		gpio-pwr = <&gpio_ccm 0 0>;
		gpio-event = <&gpio_ccm 1 0>;
	};

	/* Bluetooth that uses the ASIU GPIO 5, with polarity inverted */
	bluetooth {
		...
		...
		bcm,rfkill-bank-sel = <&gpio_asiu 5 1>
	}
