* Freescale Fast Ethernet Controller (FEC)

Required properties:
- compatible : Should be "fsl,<soc>-fec"
- reg : Address and length of the register set for the device
- interrupts : Should contain fec interrupt
- phy-mode : See ethernet.txt file in the same directory

Optional properties:
- phy-reset-gpios : Should specify the gpio for phy reset
- phy-reset-duration : Reset duration in milliseconds.  Should present
  only if property "phy-reset-gpios" is available.  Missing the property
  will have the duration be 1 millisecond.  Numbers greater than 1000 are
  invalid and 1 millisecond will be used instead.
- phy-supply : regulator that powers the Ethernet PHY.
- phy-handle : phandle to the PHY device connected to this device.
- fixed-link : Assume a fixed link. See fixed-link.txt in the same directory.
  Use instead of phy-handle.
- fsl,num-tx-queues : The property is valid for enet-avb IP, which supports
  hw multi queues. Should specify the tx queue number, otherwise set tx queue
  number to 1.
- fsl,num-rx-queues : The property is valid for enet-avb IP, which supports
  hw multi queues. Should specify the rx queue number, otherwise set rx queue
  number to 1.
- fsl,magic-packet : If present, indicates that the hardware supports waking
  up via magic packet.

Optional subnodes:
- mdio : specifies the mdio bus in the FEC, used as a container for phy nodes
  according to phy.txt in the same directory

Example:

ethernet@83fec000 {
	compatible = "fsl,imx51-fec", "fsl,imx27-fec";
	reg = <0x83fec000 0x4000>;
	interrupts = <87>;
	phy-mode = "mii";
	phy-reset-gpios = <&gpio2 14 0>; /* GPIO2_14 */
	local-mac-address = [00 04 9F 01 1B B9];
	phy-supply = <&reg_fec_supply>;
};

Example with phy specified:

ethernet@83fec000 {
	compatible = "fsl,imx51-fec", "fsl,imx27-fec";
	reg = <0x83fec000 0x4000>;
	interrupts = <87>;
	phy-mode = "mii";
	phy-reset-gpios = <&gpio2 14 0>; /* GPIO2_14 */
	local-mac-address = [00 04 9F 01 1B B9];
	phy-supply = <&reg_fec_supply>;
	phy-handle = <&ethphy>;
	mdio {
		ethphy: ethernet-phy@6 {
			compatible = "ethernet-phy-ieee802.3-c22";
			reg = <6>;
			max-speed = <100>;
		};
	};
};
