Shanghai AVIC Optoelectronics 7" 1024x600 color TFT-LCD panel

Required properties:
- compatible: should be "avic,tm070ddh03"

This binding is compatible with the simple-panel binding, which is specified
in simple-panel.txt in this directory.
