Samsung SoC SSS (Security SubSystem) module

The SSS module in S5PV210 SoC supports the following:
-- Feeder (FeedCtrl)
-- Advanced Encryption Standard (AES)
-- Data Encryption Standard (DES)/3DES
-- Public Key Accelerator (PKA)
-- SHA-1/SHA-256/MD5/HMAC (SHA-1/SHA-256/MD5)/PRNG
-- PRNG: Pseudo Random Number Generator

The SSS module in Exynos4 (Exynos4210) and
Exynos5 (Exynos5420 and Exynos5250) SoCs
supports the following also:
-- ARCFOUR (ARC4)
-- True Random Number Generator (TRNG)
-- Secure Key Manager

Required properties:

- compatible : Should contain entries for this and backward compatible
  SSS versions:
  - "samsung,s5pv210-secss" for S5PV210 SoC.
  - "samsung,exynos4210-secss" for Exynos4210, Exynos4212, Exynos4412, Exynos5250,
		Exynos5260 and Exynos5420 SoCs.
- reg : Offset and length of the register set for the module
- interrupts : interrupt specifiers of SSS module interrupts, should contain
		following entries:
		- first : feed control interrupt (required for all variants),
		- second : hash interrupt (required only for samsung,s5pv210-secss).

- clocks : list of clock phandle and specifier pairs for all clocks  listed in
		clock-names property.
- clock-names : list of device clock input names; should contain one entry
		"secss".
