* Renesas VSP1 Video Processing Engine

The VSP1 is a video processing engine that supports up-/down-scaling, alpha
blending, color space conversion and various other image processing features.
It can be found in the Renesas R-Car second generation SoCs.

Required properties:

  - compatible: Must contain "renesas,vsp1"

  - reg: Base address and length of the registers block for the VSP1.
  - interrupts: VSP1 interrupt specifier.
  - clocks: A phandle + clock-specifier pair for the VSP1 functional clock.

  - renesas,#rpf: Number of Read Pixel Formatter (RPF) modules in the VSP1.
  - renesas,#uds: Number of Up Down Scaler (UDS) modules in the VSP1.
  - renesas,#wpf: Number of Write Pixel Formatter (WPF) modules in the VSP1.


Optional properties:

  - renesas,has-lif: Boolean, indicates that the LCD Interface (LIF) module is
    available.
  - renesas,has-lut: Boolean, indicates that the Look Up Table (LUT) module is
    available.
  - renesas,has-sru: Boolean, indicates that the Super Resolution Unit (SRU)
    module is available.


Example: R8A7790 (R-Car H2) VSP1-S node

	vsp1@fe928000 {
		compatible = "renesas,vsp1";
		reg = <0 0xfe928000 0 0x8000>;
		interrupts = <0 267 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&mstp1_clks R8A7790_CLK_VSP1_S>;

		renesas,has-lut;
		renesas,has-sru;
		renesas,#rpf = <5>;
		renesas,#uds = <3>;
		renesas,#wpf = <4>;
	};
