Amlogic Meson6 SoCs Timer Controller

Required properties:

- compatible : should be "amlogic,meson6-timer"
- reg : Specifies base physical address and size of the registers.
- interrupts : The interrupt of the first timer

Example:

timer@c1109940 {
	compatible = "amlogic,meson6-timer";
	reg = <0xc1109940 0x14>;
	interrupts = <0 10 1>;
};
