* Clock bindings for Freescale i.MX6 SoloLite

Required properties:
- compatible: Should be "fsl,imx6sl-ccm"
- reg: Address and length of the register set
- #clock-cells: Should be <1>

The clock consumer should specify the desired clock by having the clock
ID in its "clocks" phandle cell.  See include/dt-bindings/clock/imx6sl-clock.h
for the full list of i.MX6 SoloLite clock IDs.
