* Xilinx AXI PCIe Root Port Bridge DT description

Required properties:
- #address-cells: Address representation for root ports, set to <3>
- #size-cells: Size representation for root ports, set to <2>
- #interrupt-cells: specifies the number of cells needed to encode an
	interrupt source. The value must be 1.
- compatible: Should contain "xlnx,axi-pcie-host-1.00.a"
- reg: Should contain AXI PCIe registers location and length
- device_type: must be "pci"
- interrupts: Should contain AXI PCIe interrupt
- interrupt-map-mask,
  interrupt-map: standard PCI properties to define the mapping of the
	PCI interface to interrupt numbers.
- ranges: ranges for the PCI memory regions (I/O space region is not
	supported by hardware)
	Please refer to the standard PCI bus binding document for a more
	detailed explanation

Optional properties:
- bus-range: PCI bus numbers covered

Interrupt controller child node
+++++++++++++++++++++++++++++++
Required properties:
- interrupt-controller: identifies the node as an interrupt controller
- #address-cells: specifies the number of cells needed to encode an
	address. The value must be 0.
- #interrupt-cells: specifies the number of cells needed to encode an
	interrupt source. The value must be 1.

NOTE:
The core provides a single interrupt for both INTx/MSI messages. So,
created a interrupt controller node to support 'interrupt-map' DT
functionality.  The driver will create an IRQ domain for this map, decode
the four INTx interrupts in ISR and route them to this domain.


Example:
++++++++

	pci_express: axi-pcie@50000000 {
		#address-cells = <3>;
		#size-cells = <2>;
		#interrupt-cells = <1>;
		compatible = "xlnx,axi-pcie-host-1.00.a";
		reg = < 0x50000000 0x10000000 >;
		device_type = "pci";
		interrupts = < 0 52 4 >;
		interrupt-map-mask = <0 0 0 7>;
		interrupt-map = <0 0 0 1 &pcie_intc 1>,
				<0 0 0 2 &pcie_intc 2>,
				<0 0 0 3 &pcie_intc 3>,
				<0 0 0 4 &pcie_intc 4>;
		ranges = < 0x02000000 0 0x60000000 0x60000000 0 0x10000000 >;

		pcie_intc: interrupt-controller {
			interrupt-controller;
			#address-cells = <0>;
			#interrupt-cells = <1>;
		};
	};
