DMAengine controller documentation
==================================

Hardware Introduction
+++++++++++++++++++++

Most of the Slave DMA controllers have the same general principles of
operations.

They have a given number of channels to use for the DMA transfers, and
a given number of requests lines.

Requests and channels are pretty much orthogonal. Channels can be used
to serve several to any requests. To simplify, channels are the
entities that will be doing the copy, and requests what endpoints are
involved.

The request lines actually correspond to physical lines going from the
DMA-eligible devices to the controller itself. Whenever the device
will want to start a transfer, it will assert a DMA request (DRQ) by
asserting that request line.

A very simple DMA controller would only take into account a single
parameter: the transfer size. At each clock cycle, it would transfer a
byte of data from one buffer to another, until the transfer size has
been reached.

That wouldn't work well in the real world, since slave devices might
require a specific number of bits to be transferred in a single
cycle. For example, we may want to transfer as much data as the
physical bus allows to maximize performances when doing a simple
memory copy operation, but our audio device could have a narrower FIFO
that requires data to be written exactly 16 or 24 bits at a time. This
is why most if not all of the DMA controllers can adjust this, using a
parameter called the transfer width.

Moreover, some DMA controllers, whenever the RAM is used as a source
or destination, can group the reads or writes in memory into a buffer,
so instead of having a lot of small memory accesses, which is not
really efficient, you'll get several bigger transfers. This is done
using a parameter called the burst size, that defines how many single
reads/writes it's allowed to do without the controller splitting the
transfer into smaller sub-transfers.

Our theoretical DMA controller would then only be able to do transfers
that involve a single contiguous block of data. However, some of the
transfers we usually have are not, and want to copy data from
non-contiguous buffers to a contiguous buffer, which is called
scatter-gather.

DMAEngine, at least for mem2dev transfers, require support for
scatter-gather. So we're left with two cases here: either we have a
quite simple DMA controller that doesn't support it, and we'll have to
implement it in software, or we have a more advanced DMA controller,
that implements in hardware scatter-gather.

The latter are usually programmed using a collection of chunks to
transfer, and whenever the transfer is started, the controller will go
over that collection, doing whatever we programmed there.

This collection is usually either a table or a linked list. You will
then push either the address of the table and its number of elements,
or the first item of the list to one channel of the DMA controller,
and whenever a DRQ will be asserted, it will go through the collection
to know where to fetch the data from.

Either way, the format of this collection is completely dependent on
your hardware. Each DMA controller will require a different structure,
but all of them will require, for every chunk, at least the source and
destination addresses, whether it should increment these addresses or
not and the three parameters we saw earlier: the burst size, the
transfer width and the transfer size.

The one last thing is that usually, slave devices won't issue DRQ by
default, and you have to enable this in your slave device driver first
whenever you're willing to use DMA.

These were just the general memory-to-memory (also called mem2mem) or
memory-to-device (mem2dev) kind of transfers. Most devices often
support other kind of transfers or memory operations that dmaengine
support and will be detailed later in this document.

DMA Support in Linux
++++++++++++++++++++

Historically, DMA controller drivers have been implemented using the
async TX API, to offload operations such as memory copy, XOR,
cryptography, etc., basically any memory to memory operation.

Over time, the need for memory to device transfers arose, and
dmaengine was extended. Nowadays, the async TX API is written as a
layer on top of dmaengine, and acts as a client. Still, dmaengine
accommodates that API in some cases, and made some design choices to
ensure that it stayed compatible.

For more information on the Async TX API, please look the relevant
documentation file in Documentation/crypto/async-tx-api.txt.

DMAEngine Registration
++++++++++++++++++++++

struct dma_device Initialization
--------------------------------

Just like any other kernel framework, the whole DMAEngine registration
relies on the driver filling a structure and registering against the
framework. In our case, that structure is dma_device.

The first thing you need to do in your driver is to allocate this
structure. Any of the usual memory allocators will do, but you'll also
need to initialize a few fields in there:

  * channels:	should be initialized as a list using the
		INIT_LIST_HEAD macro for example

  * src_addr_widths:
    - should contain a bitmask of the supported source transfer width

  * dst_addr_widths:
    - should contain a bitmask of the supported destination transfer
      width

  * directions:
    - should contain a bitmask of the supported slave directions
      (i.e. excluding mem2mem transfers)

  * residue_granularity:
    - Granularity of the transfer residue reported to dma_set_residue.
    - This can be either:
      + Descriptor
        -> Your device doesn't support any kind of residue
           reporting. The framework will only know that a particular
           transaction descriptor is done.
      + Segment
        -> Your device is able to report which chunks have been
           transferred
      + Burst
        -> Your device is able to report which burst have been
           transferred

  * dev: 	should hold the pointer to the struct device associated
		to your current driver instance.

Supported transaction types
---------------------------

The next thing you need is to set which transaction types your device
(and driver) supports.

Our dma_device structure has a field called cap_mask that holds the
various types of transaction supported, and you need to modify this
mask using the dma_cap_set function, with various flags depending on
transaction types you support as an argument.

All those capabilities are defined in the dma_transaction_type enum,
in include/linux/dmaengine.h

Currently, the types available are:
  * DMA_MEMCPY
    - The device is able to do memory to memory copies

  * DMA_XOR
    - The device is able to perform XOR operations on memory areas
    - Used to accelerate XOR intensive tasks, such as RAID5

  * DMA_XOR_VAL
    - The device is able to perform parity check using the XOR
      algorithm against a memory buffer.

  * DMA_PQ
    - The device is able to perform RAID6 P+Q computations, P being a
      simple XOR, and Q being a Reed-Solomon algorithm.

  * DMA_PQ_VAL
    - The device is able to perform parity check using RAID6 P+Q
      algorithm against a memory buffer.

  * DMA_INTERRUPT
    - The device is able to trigger a dummy transfer that will
      generate periodic interrupts
    - Used by the client drivers to register a callback that will be
      called on a regular basis through the DMA controller interrupt

  * DMA_SG
    - The device supports memory to memory scatter-gather
      transfers.
    - Even though a plain memcpy can look like a particular case of a
      scatter-gather transfer, with a single chunk to transfer, it's a
      distinct transaction type in the mem2mem transfers case

  * DMA_PRIVATE
    - The devices only supports slave transfers, and as such isn't
      available for async transfers.

  * DMA_ASYNC_TX
    - Must not be set by the device, and will be set by the framework
      if needed
    - /* TODO: What is it about? */

  * DMA_SLAVE
    - The device can handle device to memory transfers, including
      scatter-gather transfers.
    - While in the mem2mem case we were having two distinct types to
      deal with a single chunk to copy or a collection of them, here,
      we just have a single transaction type that is supposed to
      handle both.
    - If you want to transfer a single contiguous memory buffer,
      simply build a scatter list with only one item.

  * DMA_CYCLIC
    - The device can handle cyclic transfers.
    - A cyclic transfer is a transfer where the chunk collection will
      loop over itself, with the last item pointing to the first.
    - It's usually used for audio transfers, where you want to operate
      on a single ring buffer that you will fill with your audio data.

  * DMA_INTERLEAVE
    - The device supports interleaved transfer.
    - These transfers can transfer data from a non-contiguous buffer
      to a non-contiguous buffer, opposed to DMA_SLAVE that can
      transfer data from a non-contiguous data set to a continuous
      destination buffer.
    - It's usually used for 2d content transfers, in which case you
      want to transfer a portion of uncompressed data directly to the
      display to print it

These various types will also affect how the source and destination
addresses change over time.

Addresses pointing to RAM are typically incremented (or decremented)
after each transfer. In case of a ring buffer, they may loop
(DMA_CYCLIC). Addresses pointing to a device's register (e.g. a FIFO)
are typically fixed.

Device operations
-----------------

Our dma_device structure also requires a few function pointers in
order to implement the actual logic, now that we described what
operations we were able to perform.

The functions that we have to fill in there, and hence have to
implement, obviously depend on the transaction types you reported as
supported.

   * device_alloc_chan_resources
   * device_free_chan_resources
     - These functions will be called whenever a driver will call
       dma_request_channel or dma_release_channel for the first/last
       time on the channel associated to that driver.
     - They are in charge of allocating/freeing all the needed
       resources in order for that channel to be useful for your
       driver.
     - These functions can sleep.

   * device_prep_dma_*
     - These functions are matching the capabilities you registered
       previously.
     - These functions all take the buffer or the scatterlist relevant
       for the transfer being prepared, and should create a hardware
       descriptor or a list of hardware descriptors from it
     - These functions can be called from an interrupt context
     - Any allocation you might do should be using the GFP_NOWAIT
       flag, in order not to potentially sleep, but without depleting
       the emergency pool either.
     - Drivers should try to pre-allocate any memory they might need
       during the transfer setup at probe time to avoid putting to
       much pressure on the nowait allocator.

     - It should return a unique instance of the
       dma_async_tx_descriptor structure, that further represents this
       particular transfer.

     - This structure can be initialized using the function
       dma_async_tx_descriptor_init.
     - You'll also need to set two fields in this structure:
       + flags:
		TODO: Can it be modified by the driver itself, or
		should it be always the flags passed in the arguments

       + tx_submit:	A pointer to a function you have to implement,
			that is supposed to push the current
			transaction descriptor to a pending queue, waiting
			for issue_pending to be called.

   * device_issue_pending
     - Takes the first transaction descriptor in the pending queue,
       and starts the transfer. Whenever that transfer is done, it
       should move to the next transaction in the list.
     - This function can be called in an interrupt context

   * device_tx_status
     - Should report the bytes left to go over on the given channel
     - Should only care about the transaction descriptor passed as
       argument, not the currently active one on a given channel
     - The tx_state argument might be NULL
     - Should use dma_set_residue to report it
     - In the case of a cyclic transfer, it should only take into
       account the current period.
     - This function can be called in an interrupt context.

   * device_config
     - Reconfigures the channel with the configuration given as
       argument
     - This command should NOT perform synchronously, or on any
       currently queued transfers, but only on subsequent ones
     - In this case, the function will receive a dma_slave_config
       structure pointer as an argument, that will detail which
       configuration to use.
     - Even though that structure contains a direction field, this
       field is deprecated in favor of the direction argument given to
       the prep_* functions
     - This call is mandatory for slave operations only. This should NOT be
       set or expected to be set for memcpy operations.
       If a driver support both, it should use this call for slave
       operations only and not for memcpy ones.

   * device_pause
     - Pauses a transfer on the channel
     - This command should operate synchronously on the channel,
       pausing right away the work of the given channel

   * device_resume
     - Resumes a transfer on the channel
     - This command should operate synchronously on the channel,
       pausing right away the work of the given channel

   * device_terminate_all
     - Aborts all the pending and ongoing transfers on the channel
     - This command should operate synchronously on the channel,
       terminating right away all the channels

Misc notes (stuff that should be documented, but don't really know
where to put them)
------------------------------------------------------------------
  * dma_run_dependencies
    - Should be called at the end of an async TX transfer, and can be
      ignored in the slave transfers case.
    - Makes sure that dependent operations are run before marking it
      as complete.

  * dma_cookie_t
    - it's a DMA transaction ID that will increment over time.
    - Not really relevant any more since the introduction of virt-dma
      that abstracts it away.

  * DMA_CTRL_ACK
    - If set, the transfer can be reused after being completed.
    - There is a guarantee the transfer won't be freed until it is acked
      by async_tx_ack().
    - As a consequence, if a device driver wants to skip the dma_map_sg() and
      dma_unmap_sg() in between 2 transfers, because the DMA'd data wasn't used,
      it can resubmit the transfer right after its completion.

General Design Notes
--------------------

Most of the DMAEngine drivers you'll see are based on a similar design
that handles the end of transfer interrupts in the handler, but defer
most work to a tasklet, including the start of a new transfer whenever
the previous transfer ended.

This is a rather inefficient design though, because the inter-transfer
latency will be not only the interrupt latency, but also the
scheduling latency of the tasklet, which will leave the channel idle
in between, which will slow down the global transfer rate.

You should avoid this kind of practice, and instead of electing a new
transfer in your tasklet, move that part to the interrupt handler in
order to have a shorter idle window (that we can't really avoid
anyway).

Glossary
--------

Burst: 		A number of consecutive read or write operations
		that can be queued to buffers before being flushed to
		memory.
Chunk:		A contiguous collection of bursts
Transfer:	A collection of chunks (be it contiguous or not)
