* Avago APDS9300 ambient light sensor

http://www.avagotech.com/docs/AV02-1077EN

Required properties:

  - compatible : should be "avago,apds9300"
  - reg : the I2C address of the sensor

Optional properties:

  - interrupt-parent : should be the phandle for the interrupt controller
  - interrupts : interrupt mapping for GPIO IRQ

Example:

apds9300@39 {
	compatible = "avago,apds9300";
	reg = <0x39>;
	interrupt-parent = <&gpio2>;
	interrupts = <29 8>;
};
