Amlogic MesonX device tree bindings
-------------------------------------------

Boards with the Amlogic Meson6 SoC shall have the following properties:
  Required root node property:
    compatible: "amlogic,meson6"

Boards with the Amlogic Meson8 SoC shall have the following properties:
  Required root node property:
    compatible: "amlogic,meson8";

Board compatible values:
  - "geniatech,atv1200"
  - "minix,neo-x8"
