PFUZE100 family of regulators

Required properties:
- compatible: "fsl,pfuze100", "fsl,pfuze200", "fsl,pfuze3000"
- reg: I2C slave address

Required child node:
- regulators: This is the list of child nodes that specify the regulator
  initialization data for defined regulators. Please refer to below doc
  Documentation/devicetree/bindings/regulator/regulator.txt.

  The valid names for regulators are:
  --PFUZE100
  sw1ab,sw1c,sw2,sw3a,sw3b,sw4,swbst,vsnvs,vrefddr,vgen1~vgen6
  --PFUZE200
  sw1ab,sw2,sw3a,sw3b,swbst,vsnvs,vrefddr,vgen1~vgen6
  --PFUZE3000
  sw1a,sw1b,sw2,sw3,swbst,vsnvs,vrefddr,vldo1,vldo2,vccsd,v33,vldo3,vldo4

Each regulator is defined using the standard binding for regulators.

Example 1: PFUZE100

	pmic: pfuze100@08 {
		compatible = "fsl,pfuze100";
		reg = <0x08>;

		regulators {
			sw1a_reg: sw1ab {
				regulator-min-microvolt = <300000>;
				regulator-max-microvolt = <1875000>;
				regulator-boot-on;
				regulator-always-on;
				regulator-ramp-delay = <6250>;
			};

			sw1c_reg: sw1c {
				regulator-min-microvolt = <300000>;
				regulator-max-microvolt = <1875000>;
				regulator-boot-on;
				regulator-always-on;
			};

			sw2_reg: sw2 {
				regulator-min-microvolt = <800000>;
				regulator-max-microvolt = <3300000>;
				regulator-boot-on;
				regulator-always-on;
			};

			sw3a_reg: sw3a {
				regulator-min-microvolt = <400000>;
				regulator-max-microvolt = <1975000>;
				regulator-boot-on;
				regulator-always-on;
			};

			sw3b_reg: sw3b {
				regulator-min-microvolt = <400000>;
				regulator-max-microvolt = <1975000>;
				regulator-boot-on;
				regulator-always-on;
			};

			sw4_reg: sw4 {
				regulator-min-microvolt = <800000>;
				regulator-max-microvolt = <3300000>;
			};

			swbst_reg: swbst {
				regulator-min-microvolt = <5000000>;
				regulator-max-microvolt = <5150000>;
			};

			snvs_reg: vsnvs {
				regulator-min-microvolt = <1000000>;
				regulator-max-microvolt = <3000000>;
				regulator-boot-on;
				regulator-always-on;
			};

			vref_reg: vrefddr {
				regulator-boot-on;
				regulator-always-on;
			};

			vgen1_reg: vgen1 {
				regulator-min-microvolt = <800000>;
				regulator-max-microvolt = <1550000>;
			};

			vgen2_reg: vgen2 {
				regulator-min-microvolt = <800000>;
				regulator-max-microvolt = <1550000>;
			};

			vgen3_reg: vgen3 {
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <3300000>;
			};

			vgen4_reg: vgen4 {
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <3300000>;
				regulator-always-on;
			};

			vgen5_reg: vgen5 {
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <3300000>;
				regulator-always-on;
			};

			vgen6_reg: vgen6 {
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <3300000>;
				regulator-always-on;
			};
		};
	};


Example 2: PFUZE200

	pmic: pfuze200@08 {
		compatible = "fsl,pfuze200";
		reg = <0x08>;

		regulators {
			sw1a_reg: sw1ab {
				regulator-min-microvolt = <300000>;
				regulator-max-microvolt = <1875000>;
				regulator-boot-on;
				regulator-always-on;
				regulator-ramp-delay = <6250>;
			};

			sw2_reg: sw2 {
				regulator-min-microvolt = <800000>;
				regulator-max-microvolt = <3300000>;
				regulator-boot-on;
				regulator-always-on;
			};

			sw3a_reg: sw3a {
				regulator-min-microvolt = <400000>;
				regulator-max-microvolt = <1975000>;
				regulator-boot-on;
				regulator-always-on;
			};

			sw3b_reg: sw3b {
				regulator-min-microvolt = <400000>;
				regulator-max-microvolt = <1975000>;
				regulator-boot-on;
				regulator-always-on;
			};

			swbst_reg: swbst {
				regulator-min-microvolt = <5000000>;
				regulator-max-microvolt = <5150000>;
			};

			snvs_reg: vsnvs {
				regulator-min-microvolt = <1000000>;
				regulator-max-microvolt = <3000000>;
				regulator-boot-on;
				regulator-always-on;
			};

			vref_reg: vrefddr {
				regulator-boot-on;
				regulator-always-on;
			};

			vgen1_reg: vgen1 {
				regulator-min-microvolt = <800000>;
				regulator-max-microvolt = <1550000>;
			};

			vgen2_reg: vgen2 {
				regulator-min-microvolt = <800000>;
				regulator-max-microvolt = <1550000>;
			};

			vgen3_reg: vgen3 {
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <3300000>;
			};

			vgen4_reg: vgen4 {
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <3300000>;
				regulator-always-on;
			};

			vgen5_reg: vgen5 {
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <3300000>;
				regulator-always-on;
			};

			vgen6_reg: vgen6 {
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <3300000>;
				regulator-always-on;
			};
		};
	};

Example 3: PFUZE3000

	pmic: pfuze3000@08 {
		compatible = "fsl,pfuze3000";
		reg = <0x08>;

		regulators {
			sw1a_reg: sw1a {
				regulator-min-microvolt = <700000>;
				regulator-max-microvolt = <1475000>;
				regulator-boot-on;
				regulator-always-on;
				regulator-ramp-delay = <6250>;
			};
			/* use sw1c_reg to align with pfuze100/pfuze200 */
			sw1c_reg: sw1b {
				regulator-min-microvolt = <700000>;
				regulator-max-microvolt = <1475000>;
				regulator-boot-on;
				regulator-always-on;
				regulator-ramp-delay = <6250>;
			};

			sw2_reg: sw2 {
				regulator-min-microvolt = <2500000>;
				regulator-max-microvolt = <3300000>;
				regulator-boot-on;
				regulator-always-on;
			};

			sw3a_reg: sw3 {
				regulator-min-microvolt = <900000>;
				regulator-max-microvolt = <1650000>;
				regulator-boot-on;
				regulator-always-on;
			};

			swbst_reg: swbst {
				regulator-min-microvolt = <5000000>;
				regulator-max-microvolt = <5150000>;
			};

			snvs_reg: vsnvs {
				regulator-min-microvolt = <1000000>;
				regulator-max-microvolt = <3000000>;
				regulator-boot-on;
				regulator-always-on;
			};

			vref_reg: vrefddr {
				regulator-boot-on;
				regulator-always-on;
			};

			vgen1_reg: vldo1 {
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <3300000>;
				regulator-always-on;
			};

			vgen2_reg: vldo2 {
				regulator-min-microvolt = <800000>;
				regulator-max-microvolt = <1550000>;
			};

			vgen3_reg: vccsd {
				regulator-min-microvolt = <2850000>;
				regulator-max-microvolt = <3300000>;
				regulator-always-on;
			};

			vgen4_reg: v33 {
				regulator-min-microvolt = <2850000>;
				regulator-max-microvolt = <3300000>;
			};

			vgen5_reg: vldo3 {
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <3300000>;
				regulator-always-on;
			};

			vgen6_reg: vldo4 {
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <3300000>;
				regulator-always-on;
			};
		};
	};
