ROCKCHIP USB2 PHY

Required properties:
 - compatible: rockchip,rk3288-usb-phy
 - rockchip,grf : phandle to the syscon managing the "general
   register files"
 - #address-cells: should be 1
 - #size-cells: should be 0

Sub-nodes:
Each PHY should be represented as a sub-node.

Sub-nodes
required properties:
- #phy-cells: should be 0
- reg: PHY configure reg address offset in GRF
		"0x320" - for PHY attach to OTG controller
		"0x334" - for PHY attach to HOST0 controller
		"0x348" - for PHY attach to HOST1 controller

Optional Properties:
- clocks : phandle + clock specifier for the phy clocks
- clock-names: string, clock name, must be "phyclk"

Example:

usbphy: phy {
	compatible = "rockchip,rk3288-usb-phy";
	rockchip,grf = <&grf>;
	#address-cells = <1>;
	#size-cells = <0>;

	usbphy0: usb-phy0 {
		#phy-cells = <0>;
		reg = <0x320>;
	};
};
