* Samsung Exynos5260 Clock Controller

Exynos5260 has 13 clock controllers which are instantiated
independently from the device-tree. These clock controllers
generate and supply clocks to various hardware blocks within
the SoC.

Each clock is assigned an identifier and client nodes can use
this identifier to specify the clock which they consume. All
available clocks are defined as preprocessor macros in
dt-bindings/clock/exynos5260-clk.h header and can be used in
device tree sources.

External clocks:

There are several clocks that are generated outside the SoC. It
is expected that they are defined using standard clock bindings
with following clock-output-names:

 - "fin_pll" - PLL input clock from XXTI
 - "xrtcxti" - input clock from XRTCXTI
 - "ioclk_pcm_extclk" - pcm external operation clock
 - "ioclk_spdif_extclk" - spdif external operation clock
 - "ioclk_i2s_cdclk" - i2s0 codec clock

Phy clocks:

There are several clocks which are generated by specific PHYs.
These clocks are fed into the clock controller and then routed to
the hardware blocks. These clocks are defined as fixed clocks in the
driver with following names:

 - "phyclk_dptx_phy_ch3_txd_clk" - dp phy clock for channel 3
 - "phyclk_dptx_phy_ch2_txd_clk" - dp phy clock for channel 2
 - "phyclk_dptx_phy_ch1_txd_clk" - dp phy clock for channel 1
 - "phyclk_dptx_phy_ch0_txd_clk" - dp phy clock for channel 0
 - "phyclk_hdmi_phy_tmds_clko" - hdmi phy tmds clock
 - "phyclk_hdmi_phy_pixel_clko" - hdmi phy pixel clock
 - "phyclk_hdmi_link_o_tmds_clkhi" - hdmi phy for hdmi link
 - "phyclk_dptx_phy_o_ref_clk_24m" - dp phy reference clock
 - "phyclk_dptx_phy_clk_div2"
 - "phyclk_mipi_dphy_4l_m_rxclkesc0"
 - "phyclk_usbhost20_phy_phyclock" - usb 2.0 phy clock
 - "phyclk_usbhost20_phy_freeclk"
 - "phyclk_usbhost20_phy_clk48mohci"
 - "phyclk_usbdrd30_udrd30_pipe_pclk"
 - "phyclk_usbdrd30_udrd30_phyclock" - usb 3.0 phy clock

Required Properties for Clock Controller:

 - compatible: should be one of the following.
	1) "samsung,exynos5260-clock-top"
	2) "samsung,exynos5260-clock-peri"
	3) "samsung,exynos5260-clock-egl"
	4) "samsung,exynos5260-clock-kfc"
	5) "samsung,exynos5260-clock-g2d"
	6) "samsung,exynos5260-clock-mif"
	7) "samsung,exynos5260-clock-mfc"
	8) "samsung,exynos5260-clock-g3d"
	9) "samsung,exynos5260-clock-fsys"
	10) "samsung,exynos5260-clock-aud"
	11) "samsung,exynos5260-clock-isp"
	12) "samsung,exynos5260-clock-gscl"
	13) "samsung,exynos5260-clock-disp"

 - reg: physical base address of the controller and the length of
	memory mapped region.

 - #clock-cells: should be 1.

 - clocks: list of clock identifiers which are fed as the input to
	the given clock controller. Please refer the next section to find
	the input clocks for a given controller.

 - clock-names: list of names of clocks which are fed as the input
	to the given clock controller.

Input clocks for top clock controller:
	- fin_pll
	- dout_mem_pll
	- dout_bus_pll
	- dout_media_pll

Input clocks for peri clock controller:
	- fin_pll
	- ioclk_pcm_extclk
	- ioclk_i2s_cdclk
	- ioclk_spdif_extclk
	- phyclk_hdmi_phy_ref_cko
	- dout_aclk_peri_66
	- dout_sclk_peri_uart0
	- dout_sclk_peri_uart1
	- dout_sclk_peri_uart2
	- dout_sclk_peri_spi0_b
	- dout_sclk_peri_spi1_b
	- dout_sclk_peri_spi2_b
	- dout_aclk_peri_aud
	- dout_sclk_peri_spi0_b

Input clocks for egl clock controller:
	- fin_pll
	- dout_bus_pll

Input clocks for kfc clock controller:
	- fin_pll
	- dout_media_pll

Input clocks for g2d clock controller:
	- fin_pll
	- dout_aclk_g2d_333

Input clocks for mif clock controller:
	- fin_pll

Input clocks for mfc clock controller:
	- fin_pll
	- dout_aclk_mfc_333

Input clocks for g3d clock controller:
	- fin_pll

Input clocks for fsys clock controller:
	- fin_pll
	- phyclk_usbhost20_phy_phyclock
	- phyclk_usbhost20_phy_freeclk
	- phyclk_usbhost20_phy_clk48mohci
	- phyclk_usbdrd30_udrd30_pipe_pclk
	- phyclk_usbdrd30_udrd30_phyclock
	- dout_aclk_fsys_200

Input clocks for aud clock controller:
	- fin_pll
	- fout_aud_pll
	- ioclk_i2s_cdclk
	- ioclk_pcm_extclk

Input clocks for isp clock controller:
	- fin_pll
	- dout_aclk_isp1_266
	- dout_aclk_isp1_400
	- mout_aclk_isp1_266

Input clocks for gscl clock controller:
	- fin_pll
	- dout_aclk_gscl_400
	- dout_aclk_gscl_333

Input clocks for disp clock controller:
	- fin_pll
	- phyclk_dptx_phy_ch3_txd_clk
	- phyclk_dptx_phy_ch2_txd_clk
	- phyclk_dptx_phy_ch1_txd_clk
	- phyclk_dptx_phy_ch0_txd_clk
	- phyclk_hdmi_phy_tmds_clko
	- phyclk_hdmi_phy_ref_clko
	- phyclk_hdmi_phy_pixel_clko
	- phyclk_hdmi_link_o_tmds_clkhi
	- phyclk_mipi_dphy_4l_m_txbyte_clkhs
	- phyclk_dptx_phy_o_ref_clk_24m
	- phyclk_dptx_phy_clk_div2
	- phyclk_mipi_dphy_4l_m_rxclkesc0
	- phyclk_hdmi_phy_ref_cko
	- ioclk_spdif_extclk
	- dout_aclk_peri_aud
	- dout_aclk_disp_222
	- dout_sclk_disp_pixel
	- dout_aclk_disp_333

Example 1: An example of a clock controller node is listed below.

	clock_mfc: clock-controller@11090000 {
		compatible = "samsung,exynos5260-clock-mfc";
		clock = <&fin_pll>, <&clock_top TOP_DOUT_ACLK_MFC_333>;
		clock-names = "fin_pll", "dout_aclk_mfc_333";
		reg = <0x11090000 0x10000>;
		#clock-cells = <1>;
	};

Example 2: UART controller node that consumes the clock generated by the
		peri clock controller. Refer to the standard clock bindings for
		information about 'clocks' and 'clock-names' property.

	serial@12C00000 {
		compatible = "samsung,exynos4210-uart";
		reg = <0x12C00000 0x100>;
		interrupts = <0 146 0>;
		clocks = <&clock_peri PERI_PCLK_UART0>, <&clock_peri PERI_SCLK_UART0>;
		clock-names = "uart", "clk_uart_baud0";
	};

