GTM601 UMTS modem audio interface CODEC

This device has no configuration interface. Sample rate is fixed - 8kHz.

Required properties:

  - compatible : "option,gtm601"

Example:

codec: gtm601_codec {
	compatible = "option,gtm601";
};
