ZTE platforms device tree bindings
---------------------------------------

-  ZX296702 board:
    Required root node properties:
      - compatible = "zte,zx296702-ad1", "zte,zx296702"

System management required properties:
      - compatible = "zte,sysctrl"

Low power management required properties:
      - compatible = "zte,zx296702-pcu"

Bus matrix required properties:
      - compatible = "zte,zx-bus-matrix"
