* Dialog Semiconductor DA9210 Voltage Regulator

Required properties:

- compatible:	must be "dlg,da9210"
- reg:		the i2c slave address of the regulator. It should be 0x68.

Any standard regulator properties can be used to configure the single da9210
DCDC.

Example:

	da9210@68 {
		compatible = "dlg,da9210";
		reg = <0x68>;

		regulator-min-microvolt = <900000>;
		regulator-max-microvolt = <1000000>;
		regulator-boot-on;
		regulator-always-on;
	};
