Samsung S5P/EXYNOS SoC series MIPI CSI-2 receiver (MIPI CSIS)
-------------------------------------------------------------

Required properties:

- compatible	  : "samsung,s5pv210-csis" for S5PV210 (S5PC110),
		    "samsung,exynos4210-csis" for Exynos4210 (S5PC210),
		    "samsung,exynos4212-csis" for Exynos4212/Exynos4412,
		    "samsung,exynos5250-csis" for Exynos5250;
- reg		  : offset and length of the register set for the device;
- interrupts      : should contain MIPI CSIS interrupt; the format of the
		    interrupt specifier depends on the interrupt controller;
- bus-width	  : maximum number of data lanes supported (SoC specific);
- vddio-supply    : MIPI CSIS I/O and PLL voltage supply (e.g. 1.8V);
- vddcore-supply  : MIPI CSIS Core voltage supply (e.g. 1.1V);
- clocks	  : list of clock specifiers, corresponding to entries in
		    clock-names property;
- clock-names	  : must contain "csis", "sclk_csis" entries, matching entries
		    in the clocks property.

Optional properties:

- clock-frequency : The IP's main (system bus) clock frequency in Hz, default
		    value when this property is not specified is 166 MHz;
- samsung,csis-wclk : CSI-2 wrapper clock selection. If this property is present
		    external clock from CMU will be used, or the bus clock if
		    if it's not specified.

The device node should contain one 'port' child node with one child 'endpoint'
node, according to the bindings defined in Documentation/devicetree/bindings/
media/video-interfaces.txt. The following are properties specific to those nodes.

port node
---------

- reg		  : (required) must be 3 for camera C input (CSIS0) or 4 for
		    camera D input (CSIS1);

endpoint node
-------------

- data-lanes	  : (required) an array specifying active physical MIPI-CSI2
		    data input lanes and their mapping to logical lanes; the
		    array's content is unused, only its length is meaningful;

- samsung,csis-hs-settle : (optional) differential receiver (HS-RX) settle time;


Example:

	reg0: regulator@0 {
	};

	reg1: regulator@1 {
	};

/* SoC properties */

	csis_0: csis@11880000 {
		compatible = "samsung,exynos4210-csis";
		reg = <0x11880000 0x1000>;
		interrupts = <0 78 0>;
		#address-cells = <1>;
		#size-cells = <0>;
	};

/* Board properties */

	csis_0: csis@11880000 {
		clock-frequency = <166000000>;
		vddio-supply = <&reg0>;
		vddcore-supply = <&reg1>;
		port {
			reg = <3>; /* 3 - CSIS0, 4 - CSIS1 */
			csis0_ep: endpoint {
				remote-endpoint = <...>;
				data-lanes = <1>, <2>;
				samsung,csis-hs-settle = <12>;
			};
		};
	};
