TODO:
	- additional cleaning and tests
	- wait for the new configuration interface in generic HDLC layer and
	  when available, convert the driver to it

Please send patches to Krzysztof Halasa <khc@pm.waw.pl>.