digraph board {
	rankdir=TB
	n00000001 [label="{{<port0> 0} | ipu1_csi0\n/dev/v4l-subdev0 | {<port1> 1 | <port2> 2}}", shape=Mrecord, style=filled, fillcolor=green]
	n00000001:port2 -> n00000005 [style=dashed]
	n00000001:port1 -> n0000000f:port0 [style=dashed]
	n00000001:port1 -> n0000000b:port0 [style=dashed]
	n00000005 [label="ipu1_csi0 capture\n/dev/video0", shape=box, style=filled, fillcolor=yellow]
	n0000000b [label="{{<port0> 0 | <port1> 1} | ipu1_vdic\n/dev/v4l-subdev1 | {<port2> 2}}", shape=Mrecord, style=filled, fillcolor=green]
	n0000000b:port2 -> n0000000f:port0 [style=dashed]
	n0000000f [label="{{<port0> 0} | ipu1_ic_prp\n/dev/v4l-subdev2 | {<port1> 1 | <port2> 2}}", shape=Mrecord, style=filled, fillcolor=green]
	n0000000f:port1 -> n00000013:port0 [style=dashed]
	n0000000f:port2 -> n0000001c:port0 [style=dashed]
	n00000013 [label="{{<port0> 0} | ipu1_ic_prpenc\n/dev/v4l-subdev3 | {<port1> 1}}", shape=Mrecord, style=filled, fillcolor=green]
	n00000013:port1 -> n00000016 [style=dashed]
	n00000016 [label="ipu1_ic_prpenc capture\n/dev/video1", shape=box, style=filled, fillcolor=yellow]
	n0000001c [label="{{<port0> 0} | ipu1_ic_prpvf\n/dev/v4l-subdev4 | {<port1> 1}}", shape=Mrecord, style=filled, fillcolor=green]
	n0000001c:port1 -> n0000001f [style=dashed]
	n0000001f [label="ipu1_ic_prpvf capture\n/dev/video2", shape=box, style=filled, fillcolor=yellow]
	n0000002f [label="{{<port0> 0} | ipu1_csi1\n/dev/v4l-subdev5 | {<port1> 1 | <port2> 2}}", shape=Mrecord, style=filled, fillcolor=green]
	n0000002f:port2 -> n00000033 [style=dashed]
	n0000002f:port1 -> n0000000f:port0 [style=dashed]
	n0000002f:port1 -> n0000000b:port0 [style=dashed]
	n00000033 [label="ipu1_csi1 capture\n/dev/video3", shape=box, style=filled, fillcolor=yellow]
	n0000003d [label="{{<port0> 0} | ipu2_csi0\n/dev/v4l-subdev6 | {<port1> 1 | <port2> 2}}", shape=Mrecord, style=filled, fillcolor=green]
	n0000003d:port2 -> n00000041 [style=dashed]
	n0000003d:port1 -> n0000004b:port0 [style=dashed]
	n0000003d:port1 -> n00000047:port0 [style=dashed]
	n00000041 [label="ipu2_csi0 capture\n/dev/video4", shape=box, style=filled, fillcolor=yellow]
	n00000047 [label="{{<port0> 0 | <port1> 1} | ipu2_vdic\n/dev/v4l-subdev7 | {<port2> 2}}", shape=Mrecord, style=filled, fillcolor=green]
	n00000047:port2 -> n0000004b:port0 [style=dashed]
	n0000004b [label="{{<port0> 0} | ipu2_ic_prp\n/dev/v4l-subdev8 | {<port1> 1 | <port2> 2}}", shape=Mrecord, style=filled, fillcolor=green]
	n0000004b:port1 -> n0000004f:port0 [style=dashed]
	n0000004b:port2 -> n00000058:port0 [style=dashed]
	n0000004f [label="{{<port0> 0} | ipu2_ic_prpenc\n/dev/v4l-subdev9 | {<port1> 1}}", shape=Mrecord, style=filled, fillcolor=green]
	n0000004f:port1 -> n00000052 [style=dashed]
	n00000052 [label="ipu2_ic_prpenc capture\n/dev/video5", shape=box, style=filled, fillcolor=yellow]
	n00000058 [label="{{<port0> 0} | ipu2_ic_prpvf\n/dev/v4l-subdev10 | {<port1> 1}}", shape=Mrecord, style=filled, fillcolor=green]
	n00000058:port1 -> n0000005b [style=dashed]
	n0000005b [label="ipu2_ic_prpvf capture\n/dev/video6", shape=box, style=filled, fillcolor=yellow]
	n0000006b [label="{{<port0> 0} | ipu2_csi1\n/dev/v4l-subdev11 | {<port1> 1 | <port2> 2}}", shape=Mrecord, style=filled, fillcolor=green]
	n0000006b:port2 -> n0000006f [style=dashed]
	n0000006b:port1 -> n0000004b:port0 [style=dashed]
	n0000006b:port1 -> n00000047:port0 [style=dashed]
	n0000006f [label="ipu2_csi1 capture\n/dev/video7", shape=box, style=filled, fillcolor=yellow]
	n00000079 [label="{{<port0> 0 | <port1> 1} | ipu1_csi0_mux\n/dev/v4l-subdev12 | {<port2> 2}}", shape=Mrecord, style=filled, fillcolor=green]
	n00000079:port2 -> n00000001:port0 [style=dashed]
	n0000007d [label="{{<port0> 0 | <port1> 1} | ipu2_csi1_mux\n/dev/v4l-subdev13 | {<port2> 2}}", shape=Mrecord, style=filled, fillcolor=green]
	n0000007d:port2 -> n0000006b:port0 [style=dashed]
	n00000081 [label="{{} | adv7180 3-0021\n/dev/v4l-subdev14 | {<port0> 0}}", shape=Mrecord, style=filled, fillcolor=green]
	n00000081:port0 -> n00000079:port1 [style=dashed]
}
