<title>DVB Network API</title>
<para>The DVB net device enables feeding of MPE (multi protocol encapsulation) packets
received via DVB into the Linux network protocol stack, e.g. for internet via satellite
applications. It can be accessed through <emphasis role="tt">/dev/dvb/adapter0/net0</emphasis>. Data types and
and ioctl definitions can be accessed by including <emphasis role="tt">linux/dvb/net.h</emphasis> in your
application.
</para>
<section id="dvb_net_types">
<title>DVB Net Data Types</title>

<section id="dvb-net-if">
<title>struct dvb_net_if</title>
<programlisting>
struct dvb_net_if {
	__u16 pid;
	__u16 if_num;
	__u8  feedtype;
#define DVB_NET_FEEDTYPE_MPE 0	/&#x22C6; multi protocol encapsulation &#x22C6;/
#define DVB_NET_FEEDTYPE_ULE 1	/&#x22C6; ultra lightweight encapsulation &#x22C6;/
};
</programlisting>
</section>

</section>
<section id="net_fcalls">
<title>DVB net Function Calls</title>
<para>To be written&#x2026;
</para>
</section>
