Marvell Platforms Device Tree Bindings
----------------------------------------------------

PXA168 Aspenite Board
Required root node properties:
	- compatible = "mrvl,pxa168-aspenite", "mrvl,pxa168";

PXA910 DKB Board
Required root node properties:
	- compatible = "mrvl,pxa910-dkb";

MMP2 Brownstone Board
Required root node properties:
	- compatible = "mrvl,mmp2-brownstone";
