RK8XX Power Management Integrated Circuit

The rk8xx family current members:
rk805
rk808
rk809
rk817
rk818

Required properties:
- compatible: "rockchip,rk805"
- compatible: "rockchip,rk808"
- compatible: "rockchip,rk809"
- compatible: "rockchip,rk817"
- compatible: "rockchip,rk818"
- reg: I2C slave address
- interrupts: the interrupt outputs of the controller.
- #clock-cells: from common clock binding; shall be set to 1 (multiple clock
  outputs). See <dt-bindings/clock/rockchip,rk808.h> for clock IDs.

Optional properties:
- clock-output-names: From common clock binding to override the
  default output clock name
- rockchip,system-power-controller: Telling whether or not this pmic is controlling
  the system power.
- wakeup-source: Device can be used as a wakeup source.

Optional RK805 properties:
- vcc1-supply:  The input supply for DCDC_REG1
- vcc2-supply:  The input supply for DCDC_REG2
- vcc3-supply:  The input supply for DCDC_REG3
- vcc4-supply:  The input supply for DCDC_REG4
- vcc5-supply:  The input supply for LDO_REG1 and LDO_REG2
- vcc6-supply:  The input supply for LDO_REG3

Optional RK808 properties:
- vcc1-supply:  The input supply for DCDC_REG1
- vcc2-supply:  The input supply for DCDC_REG2
- vcc3-supply:  The input supply for DCDC_REG3
- vcc4-supply:  The input supply for DCDC_REG4
- vcc6-supply:  The input supply for LDO_REG1 and LDO_REG2
- vcc7-supply:  The input supply for LDO_REG3 and LDO_REG7
- vcc8-supply:  The input supply for SWITCH_REG1
- vcc9-supply:  The input supply for LDO_REG4 and LDO_REG5
- vcc10-supply: The input supply for LDO_REG6
- vcc11-supply: The input supply for LDO_REG8
- vcc12-supply: The input supply for SWITCH_REG2
- dvs-gpios:  buck1/2 can be controlled by gpio dvs, this is GPIO specifiers
  for 2 host gpio's used for dvs. The format of the gpio specifier depends in
  the gpio controller. If DVS GPIOs aren't present, voltage changes will happen
  very quickly with no slow ramp time.

Optional shared RK809 and RK817 properties:
- vcc1-supply:  The input supply for DCDC_REG1
- vcc2-supply:  The input supply for DCDC_REG2
- vcc3-supply:  The input supply for DCDC_REG3
- vcc4-supply:  The input supply for DCDC_REG4
- vcc5-supply:  The input supply for LDO_REG1, LDO_REG2, LDO_REG3
- vcc6-supply:  The input supply for LDO_REG4, LDO_REG5, LDO_REG6
- vcc7-supply:  The input supply for LDO_REG7, LDO_REG8, LDO_REG9

Optional RK809 properties:
- vcc8-supply:  The input supply for SWITCH_REG1
- vcc9-supply:  The input supply for DCDC_REG5, SWITCH_REG2

Optional RK817 properties:
- clocks:	The input clock for the audio codec
- clock-names:	The clock name for the codec clock. Should be "mclk".
- #sound-dai-cells: Needed for the interpretation of sound dais. Should be 0.

- vcc8-supply:  The input supply for BOOST
- vcc9-supply:  The input supply for OTG_SWITCH
- codec:	The child node for the codec to hold additional properties.
		If no additional properties are required for the codec, this
		node can be omitted.

- rockchip,mic-in-differential: Telling if the microphone uses differential
				mode. Should be under the codec child node.

Optional RK818 properties:
- vcc1-supply:  The input supply for DCDC_REG1
- vcc2-supply:  The input supply for DCDC_REG2
- vcc3-supply:  The input supply for DCDC_REG3
- vcc4-supply:  The input supply for DCDC_REG4
- boost-supply: The input supply for DCDC_BOOST
- vcc6-supply:  The input supply for LDO_REG1 and LDO_REG2
- vcc7-supply:  The input supply for LDO_REG3, LDO_REG5 and LDO_REG7
- vcc8-supply:  The input supply for LDO_REG4, LDO_REG6 and LDO_REG8
- vcc9-supply:  The input supply for LDO_REG9 and SWITCH_REG
- h_5v-supply:  The input supply for HDMI_SWITCH
- usb-supply:   The input supply for OTG_SWITCH

Regulators: All the regulators of RK8XX to be instantiated shall be
listed in a child node named 'regulators'. Each regulator is represented
by a child node of the 'regulators' node.

	regulator-name {
		/* standard regulator bindings here */
	};

Following regulators of the RK805 PMIC regulators are supported. Note that
the 'n' in regulator name, as in DCDC_REGn or LDOn, represents the DCDC or LDO
number as described in RK805 datasheet.

	- DCDC_REGn
		- valid values for n are 1 to 4.
	- LDO_REGn
		- valid values for n are 1 to 3

Following regulators of the RK808 PMIC block are supported. Note that
the 'n' in regulator name, as in DCDC_REGn or LDOn, represents the DCDC or LDO
number as described in RK808 datasheet.

	- DCDC_REGn
		- valid values for n are 1 to 4.
	- LDO_REGn
		- valid values for n are 1 to 8.
	- SWITCH_REGn
		- valid values for n are 1 to 2

Following regulators of the RK809 and RK817 PMIC blocks are supported. Note that
the 'n' in regulator name, as in DCDC_REGn or LDOn, represents the DCDC or LDO
number as described in RK809 and RK817 datasheets.

	- DCDC_REGn
		- valid values for n are 1 to 5 for RK809.
		- valid values for n are 1 to 4 for RK817.
	- LDO_REGn
		- valid values for n are 1 to 9 for RK809.
		- valid values for n are 1 to 9 for RK817.
	- SWITCH_REGn
		- valid values for n are 1 to 2 for RK809.
	- BOOST for RK817
	- OTG_SWITCH for RK817

Following regulators of the RK818 PMIC block are supported. Note that
the 'n' in regulator name, as in DCDC_REGn or LDOn, represents the DCDC or LDO
number as described in RK818 datasheet.

	- DCDC_REGn
		- valid values for n are 1 to 4.
	- LDO_REGn
		- valid values for n are 1 to 9.
	- SWITCH_REG
	- HDMI_SWITCH
	- OTG_SWITCH

It is necessary to configure three pins for both the RK809 and RK817, the three
pins are "gpio_ts" "gpio_gt" "gpio_slp".
	The gpio_gt and gpio_ts pins support the gpio function.
	The gpio_slp pin is for controlling the pmic states, as below:
		- reset
		- power down
		- sleep

Standard regulator bindings are used inside regulator subnodes. Check
  Documentation/devicetree/bindings/regulator/regulator.txt
for more details

Example:
	rk808: pmic@1b {
		compatible = "rockchip,rk808";
		clock-output-names = "xin32k", "rk808-clkout2";
		interrupt-parent = <&gpio0>;
		interrupts = <4 IRQ_TYPE_LEVEL_LOW>;
		pinctrl-names = "default";
		pinctrl-0 = <&pmic_int &dvs_1 &dvs_2>;
		dvs-gpios = <&gpio7 11 GPIO_ACTIVE_HIGH>,
			    <&gpio7 15 GPIO_ACTIVE_HIGH>;
		reg = <0x1b>;
		rockchip,system-power-controller;
		wakeup-source;
		#clock-cells = <1>;

		vcc8-supply = <&vcc_18>;
		vcc9-supply = <&vcc_io>;
		vcc10-supply = <&vcc_io>;
		vcc12-supply = <&vcc_io>;
		vddio-supply = <&vccio_pmu>;

		regulators {
			vdd_cpu: DCDC_REG1 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <750000>;
				regulator-max-microvolt = <1300000>;
				regulator-name = "vdd_arm";
			};

			vdd_gpu: DCDC_REG2 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <850000>;
				regulator-max-microvolt = <1250000>;
				regulator-name = "vdd_gpu";
			};

			vcc_ddr: DCDC_REG3 {
				regulator-always-on;
				regulator-boot-on;
				regulator-name = "vcc_ddr";
			};

			vcc_io: DCDC_REG4 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <3300000>;
				regulator-max-microvolt = <3300000>;
				regulator-name = "vcc_io";
			};

			vccio_pmu: LDO_REG1 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <3300000>;
				regulator-max-microvolt = <3300000>;
				regulator-name = "vccio_pmu";
			};

			vcc_tp: LDO_REG2 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <3300000>;
				regulator-max-microvolt = <3300000>;
				regulator-name = "vcc_tp";
			};

			vdd_10: LDO_REG3 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1000000>;
				regulator-max-microvolt = <1000000>;
				regulator-name = "vdd_10";
			};

			vcc18_lcd: LDO_REG4 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
				regulator-name = "vcc18_lcd";
			};

			vccio_sd: LDO_REG5 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <3300000>;
				regulator-name = "vccio_sd";
			};

			vdd10_lcd: LDO_REG6 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1000000>;
				regulator-max-microvolt = <1000000>;
				regulator-name = "vdd10_lcd";
			};

			vcc_18: LDO_REG7 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
				regulator-name = "vcc_18";
			};

			vcca_codec: LDO_REG8 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <3300000>;
				regulator-max-microvolt = <3300000>;
				regulator-name = "vcca_codec";
			};

			vcc_wl: SWITCH_REG1 {
				regulator-always-on;
				regulator-boot-on;
				regulator-name = "vcc_wl";
			};

			vcc_lcd: SWITCH_REG2 {
				regulator-always-on;
				regulator-boot-on;
				regulator-name = "vcc_lcd";
			};
		};
	};

	rk817: pmic@20 {
		compatible = "rockchip,rk817";
		reg = <0x20>;
		interrupt-parent = <&gpio0>;
		interrupts = <RK_PB2 IRQ_TYPE_LEVEL_LOW>;
		clock-output-names = "rk808-clkout1", "xin32k";
		clock-names = "mclk";
		clocks = <&cru SCLK_I2S1_OUT>;
		pinctrl-names = "default";
		pinctrl-0 = <&pmic_int>, <&i2s1_2ch_mclk>;
		wakeup-source;
		#clock-cells = <1>;
		#sound-dai-cells = <0>;

		vcc1-supply = <&vccsys>;
		vcc2-supply = <&vccsys>;
		vcc3-supply = <&vccsys>;
		vcc4-supply = <&vccsys>;
		vcc5-supply = <&vccsys>;
		vcc6-supply = <&vccsys>;
		vcc7-supply = <&vccsys>;

		regulators {
			vdd_logic: DCDC_REG1 {
				regulator-name = "vdd_logic";
				regulator-min-microvolt = <950000>;
				regulator-max-microvolt = <1150000>;
				regulator-ramp-delay = <6001>;
				regulator-always-on;
				regulator-boot-on;

				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <950000>;
				};
			};

			vdd_arm: DCDC_REG2 {
				regulator-name = "vdd_arm";
				regulator-min-microvolt = <950000>;
				regulator-max-microvolt = <1350000>;
				regulator-ramp-delay = <6001>;
				regulator-always-on;
				regulator-boot-on;

				regulator-state-mem {
					regulator-off-in-suspend;
					regulator-suspend-microvolt = <950000>;
				};
			};

			vcc_ddr: DCDC_REG3 {
				regulator-name = "vcc_ddr";
				regulator-always-on;
				regulator-boot-on;

				regulator-state-mem {
					regulator-on-in-suspend;
				};
			};

			vcc_3v3: DCDC_REG4 {
				regulator-name = "vcc_3v3";
				regulator-min-microvolt = <3300000>;
				regulator-max-microvolt = <3300000>;
				regulator-always-on;
				regulator-boot-on;

				regulator-state-mem {
					regulator-off-in-suspend;
					regulator-suspend-microvolt = <3300000>;
				};
			};

			vcc_1v8: LDO_REG2 {
				regulator-name = "vcc_1v8";
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
				regulator-always-on;
				regulator-boot-on;

				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <1800000>;
				};
			};

			vdd_1v0: LDO_REG3 {
				regulator-name = "vdd_1v0";
				regulator-min-microvolt = <1000000>;
				regulator-max-microvolt = <1000000>;
				regulator-always-on;
				regulator-boot-on;

				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <1000000>;
				};
			};

			vcc3v3_pmu: LDO_REG4 {
				regulator-name = "vcc3v3_pmu";
				regulator-min-microvolt = <3300000>;
				regulator-max-microvolt = <3300000>;
				regulator-always-on;
				regulator-boot-on;

				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <3300000>;
				};
			};

			vccio_sd: LDO_REG5 {
				regulator-name = "vccio_sd";
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <3300000>;
				regulator-always-on;
				regulator-boot-on;

				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <3300000>;
				};
			};

			vcc_sd: LDO_REG6 {
				regulator-name = "vcc_sd";
				regulator-min-microvolt = <3300000>;
				regulator-max-microvolt = <3300000>;
				regulator-boot-on;

				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <3300000>;
				};
			};

			vcc_bl: LDO_REG7 {
				regulator-name = "vcc_bl";
				regulator-min-microvolt = <3300000>;
				regulator-max-microvolt = <3300000>;

				regulator-state-mem {
					regulator-off-in-suspend;
					regulator-suspend-microvolt = <3300000>;
				};
			};

			vcc_lcd: LDO_REG8 {
				regulator-name = "vcc_lcd";
				regulator-min-microvolt = <2800000>;
				regulator-max-microvolt = <2800000>;

				regulator-state-mem {
					regulator-off-in-suspend;
					regulator-suspend-microvolt = <2800000>;
				};
			};

			vcc_cam: LDO_REG9 {
				regulator-name = "vcc_cam";
				regulator-min-microvolt = <3000000>;
				regulator-max-microvolt = <3000000>;

				regulator-state-mem {
					regulator-off-in-suspend;
					regulator-suspend-microvolt = <3000000>;
				};
			};
		};

		rk817_codec: codec {
			rockchip,mic-in-differential;
		};
	};
