What:		/sys/devices/platform/asus_laptop/display
Date:		January 2007
KernelVersion:	2.6.20
Contact:	"Corentin Chary" <corentincj@iksaif.net>
Description:
		This file allows display switching. The value
		is composed by 4 bits and defined as follow:
		4321
		|||`- LCD
		||`-- CRT
		|`--- TV
		`---- DVI
		Ex: - 0 (0000b) means no display
		    - 3 (0011b) CRT+LCD.

What:		/sys/devices/platform/asus_laptop/gps
Date:		January 2007
KernelVersion:	2.6.20
Contact:	"Corentin Chary" <corentincj@iksaif.net>
Description:
		Control the gps device. 1 means on, 0 means off.
Users:		Lapsus

What:		/sys/devices/platform/asus_laptop/ledd
Date:		January 2007
KernelVersion:	2.6.20
Contact:	"Corentin Chary" <corentincj@iksaif.net>
Description:
		Some models like the W1N have a LED display that can be
		used to display several informations.
		To control the LED display, use the following :
		    echo 0x0T000DDD > /sys/devices/platform/asus_laptop/
		where T control the 3 letters display, and DDD the 3 digits display.
		The DDD table can be found in Documentation/laptops/asus-laptop.txt

What:		/sys/devices/platform/asus_laptop/bluetooth
Date:		January 2007
KernelVersion:	2.6.20
Contact:	"Corentin Chary" <corentincj@iksaif.net>
Description:
		Control the bluetooth device. 1 means on, 0 means off.
		This may control the led, the device or both.
Users:		Lapsus

What:		/sys/devices/platform/asus_laptop/wlan
Date:		January 2007
KernelVersion:	2.6.20
Contact:	"Corentin Chary" <corentincj@iksaif.net>
Description:
		Control the bluetooth device. 1 means on, 0 means off.
		This may control the led, the device or both.
Users:		Lapsus
