
 ==============================
 MPI Header File Change History
 ==============================

 Copyright (c) 2000-2005 LSI Logic Corporation.

 ---------------------------------------
 Header Set Release Version:    01.05.10
 Header Set Release Date:       03-11-05
 ---------------------------------------

 Filename               Current version     Prior version
 ----------             ---------------     -------------
 mpi.h                  01.05.08            01.05.07
 mpi_ioc.h              01.05.09            01.05.08
 mpi_cnfg.h             01.05.09            01.05.08
 mpi_init.h             01.05.05            01.05.04
 mpi_targ.h             01.05.05            01.05.04
 mpi_fc.h               01.05.01            01.05.01
 mpi_lan.h              01.05.01            01.05.01
 mpi_raid.h             01.05.02            01.05.02
 mpi_tool.h             01.05.03            01.05.03
 mpi_inb.h              01.05.01            01.05.01
 mpi_sas.h              01.05.01            01.05.01
 mpi_type.h             01.05.01            01.05.01
 mpi_history.txt        01.05.09            01.05.09


 *  Date      Version   Description
 *  --------  --------  ------------------------------------------------------

mpi.h
 *  05-08-00  00.10.01  Original release for 0.10 spec dated 4/26/2000.
 *  05-24-00  00.10.02  Added MPI_IOCSTATUS_SCSI_RESIDUAL_MISMATCH definition.
 *  06-06-00  01.00.01  Update MPI_VERSION_MAJOR and MPI_VERSION_MINOR.
 *  06-22-00  01.00.02  Added MPI_IOCSTATUS_LAN_ definitions.
 *                      Removed LAN_SUSPEND function definition.
 *                      Added MPI_MSGFLAGS_CONTINUATION_REPLY definition.
 *  06-30-00  01.00.03  Added MPI_CONTEXT_REPLY_TYPE_LAN definition.
 *                      Added MPI_GET/SET_CONTEXT_REPLY_TYPE macros.
 *  07-27-00  01.00.04  Added MPI_FAULT_ definitions.
 *                      Removed MPI_IOCSTATUS_MSG/DATA_XFER_ERROR definitions.
 *                      Added MPI_IOCSTATUS_INTERNAL_ERROR definition.
 *                      Added MPI_IOCSTATUS_TARGET_XFER_COUNT_MISMATCH.
 *  11-02-00  01.01.01  Original release for post 1.0 work
 *  12-04-00  01.01.02  Added new function codes.
 *  01-09-01  01.01.03  Added more definitions to the system interface section
 *                      Added MPI_IOCSTATUS_TARGET_STS_DATA_NOT_SENT.
 *  01-25-01  01.01.04  Changed MPI_VERSION_MINOR from 0x00 to 0x01.
 *  02-20-01  01.01.05  Started using MPI_POINTER.
 *                      Added defines for MPI_DIAG_PREVENT_IOC_BOOT and
 *                      MPI_DIAG_CLEAR_FLASH_BAD_SIG.
 *                      Obsoleted MPI_IOCSTATUS_TARGET_FC_ defines.
 *  02-27-01  01.01.06  Removed MPI_HOST_INDEX_REGISTER define.
 *                      Added function codes for RAID.
 *  04-09-01  01.01.07  Added alternate define for MPI_DOORBELL_ACTIVE,
 *                      MPI_DOORBELL_USED, to better match the spec.
 *  08-08-01  01.02.01  Original release for v1.2 work.
 *                      Changed MPI_VERSION_MINOR from 0x01 to 0x02.
 *                      Added define MPI_FUNCTION_TOOLBOX.
 *  09-28-01  01.02.02  New function code MPI_SCSI_ENCLOSURE_PROCESSOR.
 *  11-01-01  01.02.03  Changed name to MPI_FUNCTION_SCSI_ENCLOSURE_PROCESSOR.
 *  03-14-02  01.02.04  Added MPI_HEADER_VERSION_ defines.
 *  05-31-02  01.02.05  Bumped MPI_HEADER_VERSION_UNIT.
 *  07-12-02  01.02.06  Added define for MPI_FUNCTION_MAILBOX.
 *  09-16-02  01.02.07  Bumped value for MPI_HEADER_VERSION_UNIT.
 *  11-15-02  01.02.08  Added define MPI_IOCSTATUS_TARGET_INVALID_IO_INDEX and
 *                      obsoleted define MPI_IOCSTATUS_TARGET_INVALID_IOCINDEX.
 *  04-01-03  01.02.09  New IOCStatus code: MPI_IOCSTATUS_FC_EXCHANGE_CANCELED
 *  06-26-03  01.02.10  Bumped MPI_HEADER_VERSION_UNIT value.
 *  01-16-04  01.02.11  Added define for MPI_IOCLOGINFO_TYPE_SHIFT.
 *  04-29-04  01.02.12  Added function codes for MPI_FUNCTION_DIAG_BUFFER_POST
 *                      and MPI_FUNCTION_DIAG_RELEASE.
 *                      Added MPI_IOCSTATUS_DIAGNOSTIC_RELEASED define.
 *                      Bumped MPI_HEADER_VERSION_UNIT value.
 *  05-11-04  01.03.01  Bumped MPI_VERSION_MINOR for MPI v1.3.
 *                      Added codes for Inband.
 *  08-19-04  01.05.01  Added defines for Host Buffer Access Control doorbell.
 *                      Added define for offset of High Priority Request Queue.
 *                      Added new function codes and new IOCStatus codes.
 *                      Added a IOCLogInfo type of SAS.
 *  12-07-04  01.05.02  Bumped MPI_HEADER_VERSION_UNIT.
 *  12-09-04  01.05.03  Bumped MPI_HEADER_VERSION_UNIT.
 *  01-15-05  01.05.04  Bumped MPI_HEADER_VERSION_UNIT.
 *  02-09-05  01.05.05  Bumped MPI_HEADER_VERSION_UNIT.
 *  02-22-05  01.05.06  Bumped MPI_HEADER_VERSION_UNIT.
 *  03-11-05  01.05.07  Removed function codes for SCSI IO 32 and
 *                      TargetAssistExtended requests.
 *                      Removed EEDP IOCStatus codes.
 *  06-24-05  01.05.08  Added function codes for SCSI IO 32 and
 *                      TargetAssistExtended requests.
 *                      Added EEDP IOCStatus codes.
 *  --------------------------------------------------------------------------

mpi_ioc.h
 *  05-08-00  00.10.01  Original release for 0.10 spec dated 4/26/2000.
 *  05-24-00  00.10.02  Added _MSG_IOC_INIT_REPLY structure.
 *  06-06-00  01.00.01  Added CurReplyFrameSize field to _MSG_IOC_FACTS_REPLY.
 *  06-12-00  01.00.02  Added _MSG_PORT_ENABLE_REPLY structure.
 *                      Added _MSG_EVENT_ACK_REPLY structure.
 *                      Added _MSG_FW_DOWNLOAD_REPLY structure.
 *                      Added _MSG_TOOLBOX_REPLY structure.
 *  06-30-00  01.00.03  Added MaxLanBuckets to _PORT_FACT_REPLY structure.
 *  07-27-00  01.00.04  Added _EVENT_DATA structure definitions for _SCSI,
 *                      _LINK_STATUS, _LOOP_STATE and _LOGOUT.
 *  08-11-00  01.00.05  Switched positions of MsgLength and Function fields in
 *                      _MSG_EVENT_ACK_REPLY structure to match specification.
 *  11-02-00  01.01.01  Original release for post 1.0 work
 *                      Added a value for Manufacturer to WhoInit
 *  12-04-00  01.01.02  Modified IOCFacts reply, added FWUpload messages, and
 *                      removed toolbox message.
 *  01-09-01  01.01.03  Added event enabled and disabled defines.
 *                      Added structures for FwHeader and DataHeader.
 *                      Added ImageType to FwUpload reply.
 *  02-20-01  01.01.04  Started using MPI_POINTER.
 *  02-27-01  01.01.05  Added event for RAID status change and its event data.
 *                      Added IocNumber field to MSG_IOC_FACTS_REPLY.
 *  03-27-01  01.01.06  Added defines for ProductId field of MPI_FW_HEADER.
 *                      Added structure offset comments.
 *  04-09-01  01.01.07  Added structure EVENT_DATA_EVENT_CHANGE.
 *  08-08-01  01.02.01  Original release for v1.2 work.
 *                      New format for FWVersion and ProductId in
 *                      MSG_IOC_FACTS_REPLY and MPI_FW_HEADER.
 *  08-31-01  01.02.02  Addded event MPI_EVENT_SCSI_DEVICE_STATUS_CHANGE and
 *                      related structure and defines.
 *                      Added event MPI_EVENT_ON_BUS_TIMER_EXPIRED.
 *                      Added MPI_IOCINIT_FLAGS_DISCARD_FW_IMAGE.
 *                      Replaced a reserved field in MSG_IOC_FACTS_REPLY with
 *                      IOCExceptions and changed DataImageSize to reserved.
 *                      Added MPI_FW_DOWNLOAD_ITYPE_NVSTORE_DATA and
 *                      MPI_FW_UPLOAD_ITYPE_NVDATA.
 *  09-28-01  01.02.03  Modified Event Data for Integrated RAID.
 *  11-01-01  01.02.04  Added defines for MPI_EXT_IMAGE_HEADER ImageType field.
 *  03-14-02  01.02.05  Added HeaderVersion field to MSG_IOC_FACTS_REPLY.
 *  05-31-02  01.02.06  Added define for
 *                      MPI_IOCFACTS_EXCEPT_RAID_CONFIG_INVALID.
 *                      Added AliasIndex to EVENT_DATA_LOGOUT structure.
 *  04-01-03  01.02.07  Added defines for MPI_FW_HEADER_SIGNATURE_.
 *  06-26-03  01.02.08  Added new values to the product family defines.
 *  04-29-04  01.02.09  Added IOCCapabilities field to MSG_IOC_FACTS_REPLY and
 *                      added related defines.
 *  05-11-04  01.03.01  Original release for MPI v1.3.
 *  08-19-04  01.05.01  Added four new fields to MSG_IOC_INIT.
 *                      Added three new fields to MSG_IOC_FACTS_REPLY.
 *                      Defined four new bits for the IOCCapabilities field of
 *                      the IOCFacts reply.
 *                      Added two new PortTypes for the PortFacts reply.
 *                      Added six new events along with their EventData
 *                      structures.
 *                      Added a new MsgFlag to the FwDownload request to
 *                      indicate last segment.
 *                      Defined a new image type of boot loader.
 *                      Added FW family codes for SAS product families.
 *  10-05-04  01.05.02  Added ReplyFifoHostSignalingAddr field to
 *                      MSG_IOC_FACTS_REPLY.
 *  12-07-04  01.05.03  Added more defines for SAS Discovery Error event.
 *  12-09-04  01.05.04  Added Unsupported device to SAS Device event.
 *  01-15-05  01.05.05  Added event data for SAS SES Event.
 *  02-09-05  01.05.06  Added MPI_FW_UPLOAD_ITYPE_FW_BACKUP define.
 *  02-22-05  01.05.07  Added Host Page Buffer Persistent flag to IOC Facts
 *                      Reply and IOC Init Request.
 *  03-11-05  01.05.08  Added family code for 1068E family.
 *                      Removed IOCFacts Reply EEDP Capability bit.
 *  06-24-05  01.05.09  Added 5 new IOCFacts Reply IOCCapabilities bits.
 *                      Added Max SATA Targets to SAS Discovery Error event.
 *  --------------------------------------------------------------------------

mpi_cnfg.h
 *  05-08-00  00.10.01  Original release for 0.10 spec dated 4/26/2000.
 *  06-06-00  01.00.01  Update version number for 1.0 release.
 *  06-08-00  01.00.02  Added _PAGEVERSION definitions for all pages.
 *                      Added FcPhLowestVersion, FcPhHighestVersion, Reserved2
 *                      fields to FC_DEVICE_0 page, updated the page version.
 *                      Changed _FREE_RUNNING_CLOCK to _PACING_TRANSFERS in
 *                      SCSI_PORT_0, SCSI_DEVICE_0 and SCSI_DEVICE_1 pages
 *                      and updated the page versions.
 *                      Added _RESPONSE_ID_MASK definition to SCSI_PORT_1
 *                      page and updated the page version.
 *                      Added Information field and _INFO_PARAMS_NEGOTIATED
 *                      definitionto SCSI_DEVICE_0 page.
 *  06-22-00  01.00.03  Removed batch controls from LAN_0 page and updated the
 *                      page version.
 *                      Added BucketsRemaining to LAN_1 page, redefined the
 *                      state values, and updated the page version.
 *                      Revised bus width definitions in SCSI_PORT_0,
 *                      SCSI_DEVICE_0 and SCSI_DEVICE_1 pages.
 *  06-30-00  01.00.04  Added MaxReplySize to LAN_1 page and updated the page
 *                      version.
 *                      Moved FC_DEVICE_0 PageAddress description to spec.
 *  07-27-00  01.00.05  Corrected the SubsystemVendorID and SubsystemID field
 *                      widths in IOC_0 page and updated the page version.
 *  11-02-00  01.01.01  Original release for post 1.0 work
 *                      Added Manufacturing pages, IO Unit Page 2, SCSI SPI
 *                      Port Page 2, FC Port Page 4, FC Port Page 5
 *  12-04-00  01.01.03  Config page changes to match MPI rev 1.00.01.
 *  12-05-00  01.01.04  Modified config page actions.
 *  01-09-01  01.01.05  Added defines for page address formats.
 *                      Data size for Manufacturing pages 2 and 3 no longer
 *                      defined here.
 *                      Io Unit Page 2 size is fixed at 4 adapters and some
 *                      flags were changed.
 *                      SCSI Port Page 2 Device Settings modified.
 *                      New fields added to FC Port Page 0 and some flags
 *                      cleaned up.
 *                      Removed impedance flash from FC Port Page 1.
 *                      Added FC Port pages 6 and 7.
 *  01-25-01  01.01.06  Added MaxInitiators field to FcPortPage0.
 *  01-29-01  01.01.07  Changed some defines to make them 32 character unique.
 *                      Added some LinkType defines for FcPortPage0.
 *  02-20-01  01.01.08  Started using MPI_POINTER.
 *  02-27-01  01.01.09  Replaced MPI_CONFIG_PAGETYPE_SCSI_LUN with
 *                      MPI_CONFIG_PAGETYPE_RAID_VOLUME.
 *                      Added definitions and structures for IOC Page 2 and
 *                      RAID Volume Page 2.
 *  03-27-01  01.01.10  Added CONFIG_PAGE_FC_PORT_8 and CONFIG_PAGE_FC_PORT_9.
 *                      CONFIG_PAGE_FC_PORT_3 now supports persistent by DID.
 *                      Added VendorId and ProductRevLevel fields to
 *                      RAIDVOL2_IM_PHYS_ID struct.
 *                      Modified values for MPI_FCPORTPAGE0_FLAGS_ATTACH_
 *                      defines to make them compatible to MPI version 1.0.
 *                      Added structure offset comments.
 *  04-09-01  01.01.11  Added some new defines for the PageAddress field and
 *                      removed some obsolete ones.
 *                      Added IO Unit Page 3.
 *                      Modified defines for Scsi Port Page 2.
 *                      Modified RAID Volume Pages.
 *  08-08-01  01.02.01  Original release for v1.2 work.
 *                      Added SepID and SepBus to RVP2 IMPhysicalDisk struct.
 *                      Added defines for the SEP bits in RVP2 VolumeSettings.
 *                      Modified the DeviceSettings field in RVP2 to use the
 *                      proper structure.
 *                      Added defines for SES, SAF-TE, and cross channel for
 *                      IOCPage2 CapabilitiesFlags.
 *                      Removed define for MPI_IOUNITPAGE2_FLAGS_RAID_DISABLE.
 *                      Removed define for
 *                      MPI_SCSIPORTPAGE2_PORT_FLAGS_PARITY_ENABLE.
 *                      Added define for MPI_CONFIG_PAGEATTR_RO_PERSISTENT.
 *  08-29-01 01.02.02   Fixed value for MPI_MANUFACTPAGE_DEVID_53C1035.
 *                      Added defines for MPI_FCPORTPAGE1_FLAGS_HARD_ALPA_ONLY
 *                      and MPI_FCPORTPAGE1_FLAGS_IMMEDIATE_ERROR_REPLY.
 *                      Removed MPI_SCSIPORTPAGE0_CAP_PACING_TRANSFERS,
 *                      MPI_SCSIDEVPAGE0_NP_PACING_TRANSFERS, and
 *                      MPI_SCSIDEVPAGE1_RP_PACING_TRANSFERS, and
 *                      MPI_SCSIDEVPAGE1_CONF_PPR_ALLOWED.
 *                      Added defines for MPI_SCSIDEVPAGE1_CONF_WDTR_DISALLOWED
 *                      and MPI_SCSIDEVPAGE1_CONF_SDTR_DISALLOWED.
 *                      Added OnBusTimerValue to CONFIG_PAGE_SCSI_PORT_1.
 *                      Added rejected bits to SCSI Device Page 0 Information.
 *                      Increased size of ALPA array in FC Port Page 2 by one
 *                      and removed a one byte reserved field.
 *  09-28-01 01.02.03   Swapped NegWireSpeedLow and NegWireSpeedLow in
 *                      CONFIG_PAGE_LAN_1 to match preferred 64-bit ordering.
 *                      Added structures for Manufacturing Page 4, IO Unit
 *                      Page 3, IOC Page 3, IOC Page 4, RAID Volume Page 0, and
 *                      RAID PhysDisk Page 0.
 *  10-04-01 01.02.04   Added define for MPI_CONFIG_PAGETYPE_RAID_PHYSDISK.
 *                      Modified some of the new defines to make them 32
 *                      character unique.
 *                      Modified how variable length pages (arrays) are defined.
 *                      Added generic defines for hot spare pools and RAID
 *                      volume types.
 *  11-01-01 01.02.05   Added define for MPI_IOUNITPAGE1_DISABLE_IR.
 *  03-14-02 01.02.06   Added PCISlotNum field to CONFIG_PAGE_IOC_1 along with
 *                      related define, and bumped the page version define.
 *  05-31-02 01.02.07   Added a Flags field to CONFIG_PAGE_IOC_2_RAID_VOL in a
 *                      reserved byte and added a define.
 *                      Added define for
 *                      MPI_RAIDVOL0_STATUS_FLAG_VOLUME_INACTIVE.
 *                      Added new config page: CONFIG_PAGE_IOC_5.
 *                      Added MaxAliases, MaxHardAliases, and NumCurrentAliases
 *                      fields to CONFIG_PAGE_FC_PORT_0.
 *                      Added AltConnector and NumRequestedAliases fields to
 *                      CONFIG_PAGE_FC_PORT_1.
 *                      Added new config page: CONFIG_PAGE_FC_PORT_10.
 *  07-12-02 01.02.08   Added more MPI_MANUFACTPAGE_DEVID_ defines.
 *                      Added additional MPI_SCSIDEVPAGE0_NP_ defines.
 *                      Added more MPI_SCSIDEVPAGE1_RP_ defines.
 *                      Added define for
 *                      MPI_SCSIDEVPAGE1_CONF_EXTENDED_PARAMS_ENABLE.
 *                      Added new config page: CONFIG_PAGE_SCSI_DEVICE_3.
 *                      Modified MPI_FCPORTPAGE5_FLAGS_ defines.
 *  09-16-02 01.02.09   Added MPI_SCSIDEVPAGE1_CONF_FORCE_PPR_MSG define.
 *  11-15-02 01.02.10   Added ConnectedID defines for CONFIG_PAGE_SCSI_PORT_0.
 *                      Added more Flags defines for CONFIG_PAGE_FC_PORT_1.
 *                      Added more Flags defines for CONFIG_PAGE_FC_DEVICE_0.
 *  04-01-03 01.02.11   Added RR_TOV field and additional Flags defines for
 *                      CONFIG_PAGE_FC_PORT_1.
 *                      Added define MPI_FCPORTPAGE5_FLAGS_DISABLE to disable
 *                      an alias.
 *                      Added more device id defines.
 *  06-26-03 01.02.12   Added MPI_IOUNITPAGE1_IR_USE_STATIC_VOLUME_ID define.
 *                      Added TargetConfig and IDConfig fields to
 *                      CONFIG_PAGE_SCSI_PORT_1.
 *                      Added more PortFlags defines for CONFIG_PAGE_SCSI_PORT_2
 *                      to control DV.
 *                      Added more Flags defines for CONFIG_PAGE_FC_PORT_1.
 *                      In CONFIG_PAGE_FC_DEVICE_0, replaced Reserved1 field
 *                      with ADISCHardALPA.
 *                      Added MPI_FC_DEVICE_PAGE0_PROT_FCP_RETRY define.
 *  01-16-04  01.02.13  Added InitiatorDeviceTimeout and InitiatorIoPendTimeout
 *                      fields and related defines to CONFIG_PAGE_FC_PORT_1.
 *                      Added define for
 *                      MPI_FCPORTPAGE1_FLAGS_SOFT_ALPA_FALLBACK.
 *                      Added new fields to the substructures of
 *                      CONFIG_PAGE_FC_PORT_10.
 *  04-29-04 01.02.14   Added define for IDP bit for CONFIG_PAGE_SCSI_PORT_0,
 *                      CONFIG_PAGE_SCSI_DEVICE_0, and
 *                      CONFIG_PAGE_SCSI_DEVICE_1. Also bumped Page Version for
 *                      these pages.
 *  05-11-04 01.03.01   Added structure for CONFIG_PAGE_INBAND_0.
 *  08-19-04 01.05.01   Modified MSG_CONFIG request to support extended config
 *                      pages.
 *                      Added a new structure for extended config page header.
 *                      Added new extended config pages types and structures for
 *                      SAS IO Unit, SAS Expander, SAS Device, and SAS PHY.
 *                      Replaced a reserved byte in CONFIG_PAGE_MANUFACTURING_4
 *                      to add a Flags field.
 *                      Two new Manufacturing config pages (5 and 6).
 *                      Two new bits defined for IO Unit Page 1 Flags field.
 *                      Modified CONFIG_PAGE_IO_UNIT_2 to add three new fields
 *                      to specify the BIOS boot device.
 *                      Four new Flags bits defined for IO Unit Page 2.
 *                      Added IO Unit Page 4.
 *                      Added EEDP Flags settings to IOC Page 1.
 *                      Added new BIOS Page 1 config page.
 *  10-05-04 01.05.02   Added define for
 *                      MPI_IOCPAGE1_INITIATOR_CONTEXT_REPLY_DISABLE.
 *                      Added new Flags field to CONFIG_PAGE_MANUFACTURING_5 and
 *                      associated defines.
 *                      Added more defines for SAS IO Unit Page 0
 *                      DiscoveryStatus field.
 *                      Added define for MPI_SAS_IOUNIT0_DS_SUBTRACTIVE_LINK
 *                      and MPI_SAS_IOUNIT0_DS_TABLE_LINK.
 *                      Added defines for Physical Mapping Modes to SAS IO Unit
 *                      Page 2.
 *                      Added define for
 *                      MPI_SAS_DEVICE0_FLAGS_PORT_SELECTOR_ATTACH.
 *  10-27-04 01.05.03   Added defines for new SAS PHY page addressing mode.
 *                      Added defines for MaxTargetSpinUp to BIOS Page 1.
 *                      Added 5 new ControlFlags defines for SAS IO Unit
 *                      Page 1.
 *                      Added MaxNumPhysicalMappedIDs field to SAS IO Unit
 *                      Page 2.
 *                      Added AccessStatus field to SAS Device Page 0 and added
 *                      new Flags bits for supported SATA features.
 *  12-07-04  01.05.04  Added config page structures for BIOS Page 2, RAID
 *                      Volume Page 1, and RAID Physical Disk Page 1.
 *                      Replaced IO Unit Page 1 BootTargetID,BootBus, and
 *                      BootAdapterNum with reserved field.
 *                      Added DataScrubRate and ResyncRate to RAID Volume
 *                      Page 0.
 *                      Added MPI_SAS_IOUNIT2_FLAGS_RESERVE_ID_0_FOR_BOOT
 *                      define.
 *  12-09-04  01.05.05  Added Target Mode Large CDB Enable to FC Port Page 1
 *                      Flags field.
 *                      Added Auto Port Config flag define for SAS IOUNIT
 *                      Page 1 ControlFlags.
 *                      Added Disabled bad Phy define to Expander Page 1
 *                      Discovery Info field.
 *                      Added SAS/SATA device support to SAS IOUnit Page 1
 *                      ControlFlags.
 *                      Added Unsupported device to SAS Dev Page 0 Flags field
 *                      Added disable use SATA Hash Address for SAS IOUNIT
 *                      page 1 in ControlFields.
 *  01-15-05  01.05.06  Added defaults for data scrub rate and resync rate to
 *                      Manufacturing Page 4.
 *                      Added new defines for BIOS Page 1 IOCSettings field.
 *                      Added ExtDiskIdentifier field to RAID Physical Disk
 *                      Page 0.
 *                      Added new defines for SAS IO Unit Page 1 ControlFlags
 *                      and to SAS Device Page 0 Flags to control SATA devices.
 *                      Added defines and structures for the new Log Page 0, a
 *                      new type of configuration page.
 *  02-09-05  01.05.07  Added InactiveStatus field to RAID Volume Page 0.
 *                      Added WWID field to RAID Volume Page 1.
 *                      Added PhysicalPort field to SAS Expander pages 0 and 1.
 *  03-11-05  01.05.08  Removed the EEDP flags from IOC Page 1.
 *                      Added Enclosure/Slot boot device format to BIOS Page 2.
 *                      New status value for RAID Volume Page 0 VolumeStatus
 *                      (VolumeState subfield).
 *                      New value for RAID Physical Page 0 InactiveStatus.
 *                      Added Inactive Volume Member flag RAID Physical Disk
 *                      Page 0 PhysDiskStatus field.
 *                      New physical mapping mode in SAS IO Unit Page 2.
 *                      Added CONFIG_PAGE_SAS_ENCLOSURE_0.
 *                      Added Slot and Enclosure fields to SAS Device Page 0.
 *  06-24-05  01.05.09  Added EEDP defines to IOC Page 1.
 *                      Added more RAID type defines to IOC Page 2.
 *                      Added Port Enable Delay settings to BIOS Page 1.
 *                      Added Bad Block Table Full define to RAID Volume Page 0.
 *                      Added Previous State defines to RAID Physical Disk
 *                      Page 0.
 *                      Added Max Sata Targets define for DiscoveryStatus field
 *                      of SAS IO Unit Page 0.
 *                      Added Device Self Test to Control Flags of SAS IO Unit
 *                      Page 1.
 *                      Added Direct Attach Starting Slot Number define for SAS
 *                      IO Unit Page 2.
 *                      Added new fields in SAS Device Page 2 for enclosure
 *                      mapping.
 *                      Added OwnerDevHandle and Flags field to SAS PHY Page 0.
 *                      Added IOC GPIO Flags define to SAS Enclosure Page 0.
 *                      Fixed the value for MPI_SAS_IOUNIT1_CONTROL_DEV_SATA_SUPPORT.
 *  --------------------------------------------------------------------------

mpi_init.h
 *  05-08-00  00.10.01  Original release for 0.10 spec dated 4/26/2000.
 *  05-24-00  00.10.02  Added SenseBufferLength to _MSG_SCSI_IO_REPLY.
 *  06-06-00  01.00.01  Update version number for 1.0 release.
 *  06-08-00  01.00.02  Added MPI_SCSI_RSP_INFO_ definitions.
 *  11-02-00  01.01.01  Original release for post 1.0 work
 *  12-04-00  01.01.02  Added MPI_SCSIIO_CONTROL_NO_DISCONNECT.
 *  02-20-01  01.01.03  Started using MPI_POINTER.
 *  03-27-01  01.01.04  Added structure offset comments.
 *  04-10-01  01.01.05  Added new MsgFlag for MSG_SCSI_TASK_MGMT.
 *  08-08-01  01.02.01  Original release for v1.2 work.
 *  08-29-01  01.02.02  Added MPI_SCSITASKMGMT_TASKTYPE_LOGICAL_UNIT_RESET.
 *                      Added MPI_SCSI_STATE_QUEUE_TAG_REJECTED for
 *                      MSG_SCSI_IO_REPLY.
 *  09-28-01  01.02.03  Added structures and defines for SCSI Enclosure
 *                      Processor messages.
 *  10-04-01  01.02.04  Added defines for SEP request Action field.
 *  05-31-02  01.02.05  Added MPI_SCSIIO_MSGFLGS_CMD_DETERMINES_DATA_DIR define
 *                      for SCSI IO requests.
 *  11-15-02  01.02.06  Added special extended SCSI Status defines for FCP.
 *  06-26-03  01.02.07  Added MPI_SCSI_STATUS_FCPEXT_UNASSIGNED define.
 *  05-11-04  01.03.01  Original release for MPI v1.3.
 *  08-19-04  01.05.01  Added MsgFlags defines for EEDP to SCSI IO request.
 *                      Added new word to MSG_SCSI_IO_REPLY to add TaskTag field
 *                      and a reserved U16.
 *                      Added new MSG_SCSI_IO32_REQUEST structure.
 *                      Added a TaskType of Clear Task Set to SCSI
 *                      Task Management request.
 *  12-07-04  01.05.02  Added support for Task Management Query Task.
 *  01-15-05  01.05.03  Modified SCSI Enclosure Processor Request to support
 *                      WWID addressing.
 *  03-11-05  01.05.04  Removed EEDP flags from SCSI IO Request.
 *                      Removed SCSI IO 32 Request.
 *                      Modified SCSI Enclosure Processor Request and Reply to
 *                      support Enclosure/Slot addressing rather than WWID
 *                      addressing.
 *  06-24-05  01.05.05  Added SCSI IO 32 structures and defines.
 *                      Added four new defines for SEP SlotStatus.
 *  --------------------------------------------------------------------------

mpi_targ.h
 *  05-08-00  00.10.01  Original release for 0.10 spec dated 4/26/2000.
 *  06-06-00  01.00.01  Update version number for 1.0 release.
 *  06-22-00  01.00.02  Added _MSG_TARGET_CMD_BUFFER_POST_REPLY structure.
 *                      Corrected DECSRIPTOR typo to DESCRIPTOR.
 *  11-02-00  01.01.01  Original release for post 1.0 work
 *                      Modified target mode to use IoIndex instead of
 *                      HostIndex and IocIndex. Added Alias.
 *  01-09-01  01.01.02  Added defines for TARGET_ASSIST_FLAGS_REPOST_CMD_BUFFER
 *                      and TARGET_STATUS_SEND_FLAGS_REPOST_CMD_BUFFER.
 *  02-20-01  01.01.03  Started using MPI_POINTER.
 *                      Added structures for MPI_TARGET_SCSI_SPI_CMD_BUFFER and
 *                      MPI_TARGET_FCP_CMD_BUFFER.
 *  03-27-01  01.01.04  Added structure offset comments.
 *  08-08-01  01.02.01  Original release for v1.2 work.
 *  09-28-01  01.02.02  Added structure for MPI_TARGET_SCSI_SPI_STATUS_IU.
 *                      Added PriorityReason field to some replies and
 *                      defined more PriorityReason codes.
 *                      Added some defines for to support previous version
 *                      of MPI.
 *  10-04-01  01.02.03  Added PriorityReason to MSG_TARGET_ERROR_REPLY.
 *  11-01-01  01.02.04  Added define for TARGET_STATUS_SEND_FLAGS_HIGH_PRIORITY.
 *  03-14-02  01.02.05  Modified MPI_TARGET_FCP_RSP_BUFFER to get the proper
 *                      byte ordering.
 *  05-31-02  01.02.06  Modified TARGET_MODE_REPLY_ALIAS_MASK to only include
 *                      one bit.
 *                      Added AliasIndex field to MPI_TARGET_FCP_CMD_BUFFER.
 *  09-16-02  01.02.07  Added flags for confirmed completion.
 *                      Added PRIORITY_REASON_TARGET_BUSY.
 *  11-15-02  01.02.08  Added AliasID field to MPI_TARGET_SCSI_SPI_CMD_BUFFER.
 *  04-01-03  01.02.09  Added OptionalOxid field to MPI_TARGET_FCP_CMD_BUFFER.
 *  05-11-04  01.03.01  Original release for MPI v1.3.
 *  08-19-04  01.05.01  Added new request message structures for
 *                      MSG_TARGET_CMD_BUF_POST_BASE_REQUEST,
 *                      MSG_TARGET_CMD_BUF_POST_LIST_REQUEST, and
 *                      MSG_TARGET_ASSIST_EXT_REQUEST.
 *                      Added new structures for SAS SSP Command buffer, SSP
 *                      Task buffer, and SSP Status IU.
 *  10-05-04  01.05.02  MSG_TARGET_CMD_BUFFER_POST_BASE_LIST_REPLY added.
 *  02-22-05  01.05.03  Changed a comment.
 *  03-11-05  01.05.04  Removed TargetAssistExtended Request.
 *  06-24-05  01.05.05  Added TargetAssistExtended structures and defines.
 *  --------------------------------------------------------------------------

mpi_fc.h
 *  05-08-00  00.10.01  Original release for 0.10 spec dated 4/26/2000.
 *  06-06-00  01.00.01  Update version number for 1.0 release.
 *  06-12-00  01.00.02  Added _MSG_FC_ABORT_REPLY structure.
 *  11-02-00  01.01.01  Original release for post 1.0 work
 *  12-04-00  01.01.02  Added messages for Common Transport Send and
 *                      Primitive Send.
 *  01-09-01  01.01.03  Modifed some of the new flags to have an MPI prefix
 *                      and modified the FcPrimitiveSend flags.
 *  01-25-01  01.01.04  Move InitiatorIndex in LinkServiceRsp reply to a larger
 *                      field.
 *                      Added FC_ABORT_TYPE_CT_SEND_REQUEST and
 *                      FC_ABORT_TYPE_EXLINKSEND_REQUEST for FcAbort request.
 *                      Added MPI_FC_PRIM_SEND_FLAGS_STOP_SEND.
 *  02-20-01  01.01.05  Started using MPI_POINTER.
 *  03-27-01  01.01.06  Added Flags field to MSG_LINK_SERVICE_BUFFER_POST_REPLY
 *                      and defined MPI_LS_BUF_POST_REPLY_FLAG_NO_RSP_NEEDED.
 *                      Added MPI_FC_PRIM_SEND_FLAGS_RESET_LINK define.
 *                      Added structure offset comments.
 *  04-09-01  01.01.07  Added RspLength field to MSG_LINK_SERVICE_RSP_REQUEST.
 *  08-08-01  01.02.01  Original release for v1.2 work.
 *  09-28-01  01.02.02  Change name of reserved field in
 *                      MSG_LINK_SERVICE_RSP_REPLY.
 *  05-31-02  01.02.03  Adding AliasIndex to FC Direct Access requests.
 *  01-16-04  01.02.04  Added define for MPI_FC_PRIM_SEND_FLAGS_ML_RESET_LINK.
 *  05-11-04  01.03.01  Original release for MPI v1.3.
 *  08-19-04  01.05.01  Original release for MPI v1.5.
 *  --------------------------------------------------------------------------

mpi_lan.h
 *  05-08-00  00.10.01  Original release for 0.10 spec dated 4/26/2000.
 *  05-24-00  00.10.02  Added LANStatus field to _MSG_LAN_SEND_REPLY.
 *                      Added LANStatus field to _MSG_LAN_RECEIVE_POST_REPLY.
 *                      Moved ListCount field in _MSG_LAN_RECEIVE_POST_REPLY.
 *  06-06-00  01.00.01  Update version number for 1.0 release.
 *  06-12-00  01.00.02  Added MPI_ to BUCKETSTATUS_ definitions.
 *  06-22-00  01.00.03  Major changes to match new LAN definition in 1.0 spec.
 *  06-30-00  01.00.04  Added Context Reply definitions per revised proposal.
 *                      Changed transaction context usage to bucket/buffer.
 *  07-05-00  01.00.05  Removed LAN_RECEIVE_POST_BUCKET_CONTEXT_MASK definition
 *                      to lan private header file
 *  11-02-00  01.01.01  Original release for post 1.0 work
 *  02-20-01  01.01.02  Started using MPI_POINTER.
 *  03-27-01  01.01.03  Added structure offset comments.
 *  08-08-01  01.02.01  Original release for v1.2 work.
 *  05-11-04  01.03.01  Original release for MPI v1.3.
 *  08-19-04  01.05.01  Original release for MPI v1.5.
 *  --------------------------------------------------------------------------

mpi_raid.h
 *  02-27-01  01.01.01  Original release for this file.
 *  03-27-01  01.01.02  Added structure offset comments.
 *  08-08-01  01.02.01  Original release for v1.2 work.
 *  08-29-01  01.02.02  Added DIAG_DATA_UPLOAD_HEADER and related defines.
 *  09-28-01  01.02.02  Major rework for MPI v1.2 Integrated RAID changes.
 *  10-04-01  01.02.03  Added ActionData defines for
 *                      MPI_RAID_ACTION_DELETE_VOLUME action.
 *  11-01-01  01.02.04  Added define for MPI_RAID_ACTION_ADATA_DO_NOT_SYNC.
 *  03-14-02  01.02.05  Added define for MPI_RAID_ACTION_ADATA_LOW_LEVEL_INIT.
 *  05-07-02  01.02.06  Added define for MPI_RAID_ACTION_ACTIVATE_VOLUME,
 *                      MPI_RAID_ACTION_INACTIVATE_VOLUME, and
 *                      MPI_RAID_ACTION_ADATA_INACTIVATE_ALL.
 *  07-12-02  01.02.07  Added structures for Mailbox request and reply.
 *  11-15-02  01.02.08  Added missing MsgContext field to MSG_MAILBOX_REQUEST.
 *  04-01-03  01.02.09  New action data option flag for
 *                      MPI_RAID_ACTION_DELETE_VOLUME.
 *  05-11-04  01.03.01  Original release for MPI v1.3.
 *  08-19-04  01.05.01  Original release for MPI v1.5.
 *  01-15-05  01.05.02  Added defines for the two new RAID Actions for
 *                      _SET_RESYNC_RATE and _SET_DATA_SCRUB_RATE.
 *  --------------------------------------------------------------------------

mpi_tool.h
 *  08-08-01  01.02.01  Original release.
 *  08-29-01  01.02.02  Added DIAG_DATA_UPLOAD_HEADER and related defines.
 *  01-16-04  01.02.03  Added defines and structures for new tools
 *.                     MPI_TOOLBOX_ISTWI_READ_WRITE_TOOL and
 *                      MPI_TOOLBOX_FC_MANAGEMENT_TOOL.
 *  04-29-04  01.02.04  Added message structures for Diagnostic Buffer Post and
 *                      Diagnostic Release requests and replies.
 *  05-11-04  01.03.01  Original release for MPI v1.3.
 *  08-19-04  01.05.01  Original release for MPI v1.5.
 *  10-06-04  01.05.02  Added define for MPI_DIAG_BUF_TYPE_COUNT.
 *  02-09-05  01.05.03  Added frame size option to FC management tool.
 *                      Added Beacon tool to the Toolbox.
 *  --------------------------------------------------------------------------

mpi_inb.h
 *  05-11-04  01.03.01  Original release.
 *  08-19-04  01.05.01  Original release for MPI v1.5.
 *  --------------------------------------------------------------------------

mpi_sas.h
 *  08-19-04  01.05.01  Original release.
 *  --------------------------------------------------------------------------

mpi_type.h
 *  05-08-00  00.10.01  Original release for 0.10 spec dated 4/26/2000.
 *  06-06-00  01.00.01  Update version number for 1.0 release.
 *  11-02-00  01.01.01  Original release for post 1.0 work
 *  02-20-01  01.01.02  Added define and ifdef for MPI_POINTER.
 *  08-08-01  01.02.01  Original release for v1.2 work.
 *  05-11-04  01.03.01  Original release for MPI v1.3.
 *  08-19-04  01.05.01  Original release for MPI v1.5.
 *  --------------------------------------------------------------------------

mpi_history.txt         Parts list history

Filename    01.05.10  01.05.09
----------  --------  --------
mpi.h       01.05.08  01.05.07
mpi_ioc.h   01.05.09  01.05.08
mpi_cnfg.h  01.05.09  01.05.08
mpi_init.h  01.05.05  01.05.04
mpi_targ.h  01.05.05  01.05.04
mpi_fc.h    01.05.01  01.05.01
mpi_lan.h   01.05.01  01.05.01
mpi_raid.h  01.05.02  01.05.02
mpi_tool.h  01.05.03  01.05.03
mpi_inb.h   01.05.01  01.05.01
mpi_sas.h   01.05.01  01.05.01
mpi_type.h  01.05.01  01.05.01

Filename    01.05.08   01.05.07   01.05.06   01.05.05   01.05.04   01.05.03
----------  --------   --------   --------   --------   --------   --------
mpi.h       01.05.06   01.05.05   01.05.04   01.05.03   01.05.02   01.05.01
mpi_ioc.h   01.05.07   01.05.06   01.05.05   01.05.04   01.05.03   01.05.02
mpi_cnfg.h  01.05.07   01.05.07   01.05.06   01.05.05   01.05.04   01.05.03
mpi_init.h  01.05.03   01.05.03   01.05.03   01.05.02   01.05.02   01.05.01
mpi_targ.h  01.05.03   01.05.02   01.05.02   01.05.02   01.05.02   01.05.02
mpi_fc.h    01.05.01   01.05.01   01.05.01   01.05.01   01.05.01   01.05.01
mpi_lan.h   01.05.01   01.05.01   01.05.01   01.05.01   01.05.01   01.05.01
mpi_raid.h  01.05.02   01.05.02   01.05.02   01.05.01   01.05.01   01.05.01
mpi_tool.h  01.05.03   01.05.03   01.05.02   01.05.02   01.05.02   01.05.02
mpi_inb.h   01.05.01   01.05.01   01.05.01   01.05.01   01.05.01   01.05.01
mpi_sas.h   01.05.01   01.05.01   01.05.01   01.05.01   01.05.01   01.05.01
mpi_type.h  01.05.01   01.05.01   01.05.01   01.05.01   01.05.01   01.05.01

Filename    01.05.02   01.05.01   01.03.01   01.02.14   01.02.13   01.02.12
----------  --------   --------   --------   --------   --------   --------
mpi.h       01.05.01   01.05.01   01.03.01   01.02.12   01.02.11   01.02.10
mpi_ioc.h   01.05.02   01.05.01   01.03.01   01.02.09   01.02.08   01.02.08
mpi_cnfg.h  01.05.02   01.05.01   01.03.01   01.02.14   01.02.13   01.02.12
mpi_init.h  01.05.01   01.05.01   01.03.01   01.02.07   01.02.07   01.02.07
mpi_targ.h  01.05.02   01.05.01   01.03.01   01.02.09   01.02.09   01.02.09
mpi_fc.h    01.05.01   01.05.01   01.03.01   01.02.04   01.02.04   01.02.03
mpi_lan.h   01.05.01   01.05.01   01.03.01   01.02.01   01.02.01   01.02.01
mpi_raid.h  01.05.01   01.05.01   01.03.01   01.02.09   01.02.09   01.02.09
mpi_tool.h  01.05.02   01.05.01   01.03.01   01.02.01   01.02.01   01.02.01
mpi_inb.h   01.05.01   01.05.01   01.03.01
mpi_sas.h   01.05.01   01.05.01
mpi_type.h  01.05.01   01.05.01   01.03.01   01.02.04   01.02.03   01.02.02

Filename    01.02.11   01.02.10   01.02.09   01.02.08   01.02.07   01.02.06
----------  --------   --------   --------   --------   --------   --------
mpi.h       01.02.09   01.02.08   01.02.07   01.02.06   01.02.05   01.02.04
mpi_ioc.h   01.02.07   01.02.06   01.02.06   01.02.06   01.02.06   01.02.05
mpi_cnfg.h  01.02.11   01.02.10   01.02.09   01.02.08   01.02.07   01.02.06
mpi_init.h  01.02.06   01.02.06   01.02.05   01.02.05   01.02.05   01.02.04
mpi_targ.h  01.02.09   01.02.08   01.02.07   01.02.06   01.02.06   01.02.05
mpi_fc.h    01.02.03   01.02.03   01.02.03   01.02.03   01.02.03   01.02.02
mpi_lan.h   01.02.01   01.02.01   01.02.01   01.02.01   01.02.01   01.02.01
mpi_raid.h  01.02.09   01.02.08   01.02.07   01.02.07   01.02.06   01.02.05
mpi_tool.h  01.02.01   01.02.01   01.02.01   01.02.01   01.02.01   01.02.01
mpi_type.h  01.02.02   01.02.02   01.02.02   01.02.02   01.02.02   01.02.02

Filename    01.02.05   01.02.04   01.02.03   01.02.02   01.02.01   01.01.10
----------  --------   --------   --------   --------   --------   --------
mpi.h       01.02.03   01.02.02   01.02.02   01.02.01   01.02.01   01.01.07
mpi_ioc.h   01.02.04   01.02.03   01.02.03   01.02.02   01.02.01   01.01.07
mpi_cnfg.h  01.02.05   01.02.04   01.02.03   01.02.02   01.02.01   01.01.11
mpi_init.h  01.02.04   01.02.04   01.02.03   01.02.02   01.02.01   01.01.05
mpi_targ.h  01.02.04   01.02.03   01.02.02   01.02.01   01.02.01   01.01.04
mpi_fc.h    01.02.02   01.02.02   01.02.02   01.02.01   01.02.01   01.01.07
mpi_lan.h   01.02.01   01.02.01   01.02.01   01.02.01   01.02.01   01.01.03
mpi_raid.h  01.02.04   01.02.03   01.02.02   01.02.01   01.02.01   01.01.02
mpi_tool.h  01.02.02   01.02.02   01.02.02   01.02.02   01.02.01
mpi_type.h  01.02.02   01.02.02   01.02.02   01.02.02   01.02.01   01.01.02

Filename    01.01.09   01.01.08   01.01.07   01.01.06   01.01.05   01.01.04
----------  --------   --------   --------   --------   --------   --------
mpi.h       01.01.06   01.01.06   01.01.05   01.01.04   01.01.04   01.01.03
mpi_ioc.h   01.01.06   01.01.05   01.01.04   01.01.03   01.01.03   01.01.03
mpi_cnfg.h  01.01.10   01.01.09   01.01.08   01.01.07   01.01.06   01.01.05
mpi_init.h  01.01.04   01.01.03   01.01.03   01.01.02   01.01.02   01.01.02
mpi_targ.h  01.01.04   01.01.03   01.01.03   01.01.02   01.01.02   01.01.02
mpi_fc.h    01.01.06   01.01.05   01.01.05   01.01.04   01.01.04   01.01.03
mpi_lan.h   01.01.03   01.01.02   01.01.02   01.01.01   01.01.01   01.01.01
mpi_raid.h  01.01.02   01.01.01
mpi_type.h  01.01.02   01.01.02   01.01.02   01.01.01   01.01.01   01.01.01

Filename    01.01.03   01.01.02   01.01.01   01.00.07   01.00.06   01.00.05
----------  --------   --------   --------   --------   --------   --------
mpi.h       01.01.02   01.01.02   01.01.01   01.00.04   01.00.04   01.00.03
mpi_ioc.h   01.01.02   01.01.02   01.01.01   01.00.05   01.00.04   01.00.03
mpi_cnfg.h  01.01.04   01.01.03   01.01.01   01.00.05   01.00.05   01.00.04
mpi_init.h  01.01.02   01.01.02   01.01.01   01.00.02   01.00.02   01.00.02
mpi_targ.h  01.01.01   01.01.01   01.01.01   01.00.02   01.00.02   01.00.02
mpi_fc.h    01.01.02   01.01.02   01.01.01   01.00.02   01.00.02   01.00.02
mpi_lan.h   01.01.01   01.01.01   01.01.01   01.00.05   01.00.05   01.00.05
mpi_type.h  01.01.01   01.01.01   01.01.01   01.00.01   01.00.01   01.00.01

Filename     01.00.04   01.00.03   01.00.02   01.00.01   00.10.02   00.10.01
----------   --------   --------   --------   --------   --------   --------
mpi.h        01.00.02   01.00.01   01.00.01   01.00.01   00.10.02   00.10.01
mpi_ioc.h    01.00.02   01.00.02   01.00.01   01.00.01   00.10.02   00.10.01
mpi_cnfg.h   01.00.03   01.00.02   01.00.02   01.00.01   00.10.01   00.10.01
mpi_init.h   01.00.02   01.00.02   01.00.02   01.00.01   00.10.02   00.10.01
mpi_targ.h   01.00.02   01.00.01   01.00.01   01.00.01   00.10.01   00.10.01
mpi_fc.h     01.00.02   01.00.02   01.00.01   01.00.01   00.10.01   00.10.01
mpi_lan.h    01.00.03   01.00.02   01.00.01   01.00.01   00.10.02   00.10.01
mpi_type.h   01.00.01   01.00.01   01.00.01   01.00.01   00.10.01   00.10.01


 *  --------------------------------------------------------------------------

